{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MXM-M"]
[]
[]
[]
[]
["","","","","","5MXM90M2V1B"]
["Ventilator","Brzina protoka zraka","Hlađenje","Super nisko","m³/min","24.1"]
["","","Grijanje","Super nisko","m³/min","24.1"]
["","","","Super nisko","cfm","851"]
["","","Grijanje","Super nisko","cfm","851"]
["Dimenzije","Uređaj","","Visina","mm","734"]
["","","","Širina","mm","320"]
["","","","Dubina","mm","868"]
["Težina","Uređaj","","","kg","68"]
["Kompresor","Tip","","","","Hermetički zabrtvljen kompresor s klatnom"]
["Raspon rada","Hlađenje","Ambijent:","Min.","°CDB","-10"]
["","","","Maks.","°CDB","46"]
["","Grijanje","Ambijent:","Min.","°CWB","-15"]
["","","","Maks.","°CWB","18"]
["Razina tlaka zvuka","Hlađenje","","Nom.","dBA","52"]
["","Grijanje","","Nom.","dBA","52"]
["Radna tvar","Tip","","","","R-32"]
["","Punjenje","","","kg","2.4"]
["","Punjenje","","","tCO2Eq","1.6"]
["","GWP","","","","675"]
["Priključci cjevovoda ","Duljina cjevovoda ","Maks. ","OU - IU","m","25"]
["Priključci cjevovoda","Punjenje dodatne radne tvari","","","kg/m","0,02 (za duljinu cjevovoda koja premašuje 30 m)"]
["","Razlika razine","IU - OU","Maks.","m","15"]
["","","IU - IU","Maks.","m","7.5"]
["","Ukupna duljina cjevovoda","Sustav","Stvarno","m","75"]
["Standardna dodatna oprema","Installation manual","","","","1"]
["","Drain cap","","","","9"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Screw bag","","","","1"]
["Napajanje","Faza","","","","1~"]
["","Frekvencija","","","Hz","50"]
["","Napon","","","V","220-240"]