{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":7,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C / AZQS-BY1"]
[]
[]
[]
[]
["","","","","ABQ100CV1 / AZQS100B7Y1B","ABQ125CV1 / AZQS125B7Y1B","ABQ140CV1 / AZQS140B7Y1B"]
["Učin hlađenja","Nom.","","kW","9.5","12.1 (1)"]
["Hlađenje prostora","SEER","","","4.65","4.68"]
["","Godišnja potrošnja energije","","kWh/a","716","1,550"]
["","Kapacitet","Pdesign","kW","9.50","12.1"]
["","Razred energetske učinkovitosti","","","B"]
["Grijanje prostora (prosječna klima)","Kapacitet","Pdesign","kW","6.78","8.13"]
["","SCOP/A","","","3.80","3.41"]
["","Razred energetske učinkovitosti","","","A"]
["","Godišnja potrošnja energije","","kWh/a","2,498","3,340"]
["Nazivna učinkovitost","Godišnja potrošnja energije","","kWh","1,813"]
["","EER","","","2.62","2.27 (3)"]
["","COP","","","3.42"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","D"]
["","","Grijanje","","B"]
["Učin grijanja","Nom.","","kW","10.8","13.5 (2)"]
["Napomene","","","","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 7,5 m; razlika razine: 0 m"]
["","","","","(2) - Godišnja potrošnja energije u skladu je s direktivom oznake energetske učinkovitosti 2002/31/EC","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 7,5 m; razlika razine: 0 m"]
["","","","","(3) - SEER i SCOP su u skladu s EN 14825","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(3) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU"]
["","","","","(4) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja"]
["Učin hlađenja","Nom.","","kW","","","13.0 (1)"]
["Učin grijanja","Nom.","","kW","","","15.5 (2)"]
["Nazivna učinkovitost","EER","","","","","3.36 (3)"]
["Hlađenje prostora","Kapacitet","Pdesign","kW","","","13.0"]
["","SEER","","","","","5.01"]
["","Godišnja potrošnja energije","","kWh/a","","","1559"]
["Grijanje prostora (prosječna klima)","Kapacitet","Pdesign","kW","","","12.29"]
["","SCOP/A","","","","","3.58"]
["","Godišnja potrošnja energije","","kWh/a","","","4811"]
["Raspon energetske učinkovitosti","","","","","","A+++ ~ D"]