{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":14,"n_cols":4,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-C / ARXS-L3"]
[]
[]
[]
[]
["","","","ADEQ35C2VEB / ARXS35L3V1B"]
["Učin hlađenja","Nom.","kW","3.40 (1)"]
["Učin grijanja","Nom.","kW","4.00 (1)"]
["Napomene","","","(1) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja"]
["","","","(2) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU"]
["","","","(3) - PED: sklop = kategorija l : isključeno iz PED opsega zbog članka 1., stavke 3.6 od 97/23/EC"]
["","","","(4) - Minimalna Ssc (=Struja kratkog spoja) vrijednost: Oprema je u skladu s EN 61000-3- 2"]
["","","","(5) - Vidi električne podatke na posebnim nacrtima"]
["","","","(6) - Sadrži fluorovodične stakleničke plinove"]