{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":10,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXF-F"]
[]
[]
[]
[]
["","","","","","ARXF20F5V1B","ARXF25F5V1B","ARXF35F5V1B","ARXF42F5V1B","ARXF50F5V1B"]
["Dimenzije","Uređaj","","Visina","mm","556","556","556","556","610"]
["","","","Širina","mm","740","740","740","740","923"]
["","","","Dubina","mm","343","343","343","343","367"]
["Težina","Uređaj","","","kg","24.0","24.0","24.0","28.0","40.0"]
["Kompresor","Tip","","","","Hermetički zabrtvljen kompresor s klatnom","Hermetički zabrtvljen kompresor s klatnom","Hermetički zabrtvljen kompresor s klatnom","Hermetički zabrtvljen kompresor s klatnom","Hermetički zabrtvljen kompresor s klatnom"]
["Raspon rada","Hlađenje","Ambijent:","Min.","°CDB","-10","-10","-10","-10","-10"]
["","","","Maks.","°CDB","48","48","48","48","48"]
["","Grijanje","Ambijent:","Min.","°C WB","-15","-15","-15","-15","-15"]
["","","","Maks.","°C WB","18","18","18","18","18"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","46.0","46.0","48.0","48.0","48.0"]
["","Grijanje","","Visoko","dBA","47.0","47.0","48.0","48.0","49.0"]
["Radna tvar","Tip","","","","R-32","R-32","R-32","R-32","R-32"]
["","Punjenje","","","kg","0.420","0.420","0.500","0.750","0.800"]
["","Punjenje","","","tCO2Eq","0.280","0.280","0.340","0.510","0.540"]
["","GWP","","","","675.0","675.0","675.0","675.0","675.0"]
["Priključci cjevovoda ","Duljina cjevovoda ","Maks. ","OU - IU","m","20","20","20","20","30"]
["Priključci cjevovoda","Punjenje dodatne radne tvari","","","kg/m","002 (za duljinu cjevovoda koja premašuje 10 m)","002 (za duljinu cjevovoda koja premašuje 10 m)","002 (za duljinu cjevovoda koja premašuje 10 m)","002 (za duljinu cjevovoda koja premašuje 10 m)","002 (za duljinu cjevovoda koja premašuje 10 m)"]
["","Razlika razine","IU - OU","Maks.","m","12.0","12.0","12.0","12.0","20.0"]
["Standardna dodatna oprema","Installation manual","","","","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1"]
["","Drain plug","","","","1","1","1","1"]
["Napajanje","Faza","","","","1~","1~","1~","1~","1~"]
["","Frekvencija","","","Hz","50","50","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240","220-240","220-240"]
["Napomene","","","","","(1) - Sadrži fluorovodične stakleničke plinove","(1) - Sadrži fluorovodične stakleničke plinove","(1) - Sadrži fluorovodične stakleničke plinove","(1) - Sadrži fluorovodične stakleničke plinove","(1) - Sadrži fluorovodične stakleničke plinove"]
["","","","","","(2) - Vidi električne podatke na posebnim nacrtima","(2) - Vidi električne podatke na posebnim nacrtima","(2) - Vidi električne podatke na posebnim nacrtima","(2) - Vidi električne podatke na posebnim nacrtima","(2) - Vidi električne podatke na posebnim nacrtima"]
["","","","","","(3) - Pogledajte odvojene nacrte za radno područje","(3) - Pogledajte odvojene nacrte za radno područje","(3) - Pogledajte odvojene nacrte za radno područje","(3) - Pogledajte odvojene nacrte za radno područje","(3) - Pogledajte odvojene nacrte za radno područje"]