{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":13,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B","ARXM35R5V1B","ARXM50R2V1B","ARXM50R5V1B","ARXM60R5V1B","ARXM60R2V1B","ARXM71R5V1B","ARXM71R2V1B"]
["Dimenzije","Uređaj","","Visina","mm","550","550","734","734","734","734","734","734"]
["","","","Širina","mm","765","765","954","954","954","954","954","954"]
["","","","Dubina","mm","285","285","401","401","401","401","401","401"]
["Težina","Uređaj","","","kg","32","32","49.0","49.0","49.0","49.0","49.0","49.0"]
["Kompresor","Tip","","","","Hermetički zabrtvljen kompresor s klatnom","Hermetički zabrtvljen kompresor s klatnom","Hermetički zabrtvljen kompresor s klatnom","Hermetički zabrtvljen kompresor s klatnom","Hermetički zabrtvljen kompresor s klatnom","Hermetički zabrtvljen kompresor s klatnom","Hermetički zabrtvljen kompresor s klatnom","Hermetički zabrtvljen kompresor s klatnom"]
["Raspon rada","Hlađenje","Ambijent:","Min.","°C DB","-10","-10","-10","-10 (4) (5), -10 (4) (5)","-10","-10","-10","-10"]
["","","","Maks.","°C DB","50, 46","50, 46","50, 46","50 (4), 46 (5)","46","46","46","46"]
["","Grijanje","Ambijent:","Min.","°CWB","-15","-15","-15"]
["","","","Maks.","°CWB","18","18","18"]
["Razina tlaka zvuka","Hlađenje","","Nom.","dBA","46","49","48.0","48.0","48.0","48.0","52.0","52.0"]
["","Grijanje","","Nom.","dBA","47","49","49.0","49.0","49.0","49.0","52.0","52.0"]
["Radna tvar","Punjenje","","","kg","0.76","0.76","1.15","1.15","1.15","1.15","1.15","1.15"]
["","Punjenje","","","tCO2Eq","0.52","0.52","0.780","0.780","0.780","0.780","0.780","0.780"]
["","GWP","","","","675","675","675.0","675.0","675.0","675.0","675.0","675.0"]
["Priključci cjevovoda ","Duljina cjevovoda ","Maks. ","OU - IU","m","20","20","30","30","30","30","30","30"]
["Priključci cjevovoda","Punjenje dodatne radne tvari","","","kg/m","0,02 (za duljinu cjevovoda koja premašuje 10 m)","0,02 (za duljinu cjevovoda koja premašuje 10 m)","0,02 (za duljinu cjevovoda koja premašuje 10 m)","0,02 (za duljinu cjevovoda koja premašuje 10 m)","0,02 (za duljinu cjevovoda koja premašuje 10 m)","0,02 (za duljinu cjevovoda koja premašuje 10 m)","0,035 (za duljinu cjevovoda koja premašuje 10m)","0,035 (za duljinu cjevovoda koja premašuje 10m)"]
["","Razlika razine","IU - OU","Maks.","m","15","15","20.0","20.0","20.0","20.0","20.0","20.0"]
["Standardna dodatna oprema","Installation manual","","","","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1","1","1"]
["Napajanje","Frekvencija","","","Hz","50","50","50","50","50","50","50","50"]
["Standardna dodatna oprema","Drain cap","","","","","","3","3","3","3","3","3"]
["Napomene","","","","","","","","(1) - Moguće samo u kombinaciji s CTXM*N2V1B, ATXM*N2V1B, FTXM*N2V1B"]
["","","","","","","","","(2) - Moguće samo u kombinaciji s CTXM*M2V1B, ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9,FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB·"]