{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L3"]
[]
[]
[]
[]
["","","","","","ARXS35L3V1B","ARXS25L3V1B (Archived)"]
["Razina zvučnog tlaka","Grijanje","","Visoko","dBA","48"]
["","","","Nizak","dBA","45"]
["Standardna dodatna oprema","1","","","","550"]
["Radna tvar","Punjenje","","","kg","2.5"]
["","Tip","","","","1.2"]
["Ventilator","Količina zraka","Hlađenje","Super nisko","m³/min","30.1"]
["","","","Super nisko","cfm","1,063"]
["Fan motor","Brzina","Hlađenje","Super nisko","o/min","740"]
["","","Grijanje","Super nisko","o/min","-15"]
["Radno područje","Grijanje","Ambijent:","Min.","°C WB","20"]
["","","","Maks.","°C WB","10"]
["Razina zvučnog tlaka","Hlađenje","","Nizak","dBA","44"]
["","","","Visoko","dBA","48"]
["Kompresor","Tip","","","","Hermetički zabrtvljen kompresor s klatnom_"]
["Dimenzije","Jedinica","","Širina","mm","285"]
["","","","Dubina","mm","612"]
["","","","Height","mm","765"]
["Težina","Jedinica","","","kg","34"]
["Ventilator","Količina zraka","Grijanje","Super nisko","cfm","904"]
["","","","Super nisko","m³/min","25.6"]
["Power supply","Phase","","","","1~"]
["","Frekvencija","","","Hz","50"]
["","Napon","","","V","220-240"]
["Napomene","","","","","(1) - Sadrži fluorovodične stakleničke plinove","(1) - 220 V"]
["","","","","","(2) - 220 V","(2) - 230 V"]
["","","","","","(3) - 230 V","(3) - 240 V"]
["","","","","","(4) - 240 V"]
["Ventilator","Brzina protoka zraka","Hlađenje","Super nisko","m³/min","","30.1"]
["","","Grijanje","Super nisko","m³/min","","25.6"]
["","","","Super nisko","cfm","","1063"]
["","","Grijanje","Super nisko","cfm","","904"]
["Dimenzije","Uređaj","","Visina","mm","","550"]
["","","","Širina","mm","","765"]
["","","","Dubina","mm","","285"]
["Težina","Uređaj","","","kg","","34"]
["Motor ventilatora","Brzina","Hlađenje","Super nisko","o/min","","780"]
["","","Grijanje","Super nisko","o/min","","740"]
["Kompresor","Tip","","","","","Hermetički zabrtvljen kompresor s klatnom"]
["Raspon rada","Hlađenje","Ambijent:","Min.","°C DB","","10"]
["","","","Maks.","°C DB","","46"]
["","Grijanje","Ambijent:","Min.","°C WB","","-15"]
["","","","Maks.","°C WB","","18"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","","46"]
["","Grijanje","","Visoko","dBA","","47"]
["","","","Nizak","dBA","","44"]
["Radna tvar","Tip","","","","","R-410A"]
["","Punjenje","","","kg","","1.0"]
["","Punjenje","","","tCO2Eq","","2.1"]
["","GWP","","","","","2087.5"]
["Priključci cjevovoda ","Duljina cjevovoda ","Maks. ","OU - IU","m","","20"]
["Priključci cjevovoda","Punjenje dodatne radne tvari","","","kg/m","","0,02 (za duljinu cjevovoda koja premašuje 10 m)"]
["","Razlika razine","IU - OU","Maks.","m","","15"]
["Standardna dodatna oprema","Installation manual","","","","","1"]
["","Refrigerant charge label","","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","","1"]
["","Drain plug","","","","","1"]
["Napajanje","Faza","","","","","1~"]
["","Frekvencija","","","Hz","","50"]
["","Napon","","","V","","220-240"]