{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":8,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-E / ARXF-D"]
[]
[]
[]
[]
["","","","","ATXF20E5V1B / ARXF20D5V1B","ATXF25E5V1B / ARXF25D5V1B","ATXF35E5V1B / ARXF35D5V1B","ATXF42E5V1B / ARXF42D5V1B"]
["Cooling capacity","Min.","","kW","1.3","1.3","1.3","1.4"]
["","Maks.","","kW","2.4","2.8","3.8","4.3"]
["","Nom.","","kW","2.00","2.50","3.30","4.20"]
["Nazivna učinkovitost","Godišnja potrošnja energije","","kWh","109","137","191","228"]
["","EER","","","3.33","3.33","3.27","3.27"]
["","COP","","","3.75","3.73","3.72","3.71"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","A","A","A","A"]
["","","Grijanje","","A","A","A","A"]
["Učin grijanja","Nom.","","kW","2.40","2.80","3.50","4.60"]
["","Min.","","kW","1.30","1.30","1.30","1.40"]
["","Maks.","","kW","3.30","3.70","4.40","5.00"]
["Napomene","","","","(1) - Nazivni učini hlađenja se temelje na: unutarnjoj temperaturi: 27 °CDB, 19 °CWB, vanjskoj temperaturi: 35 °CDB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju visoke učinkovitosti, certifikat Eurovent","(1) - Nazivni učini hlađenja se temelje na: unutarnjoj temperaturi: 27 °CDB, 19 °CWB, vanjskoj temperaturi: 35 °CDB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju visoke učinkovitosti, certifikat Eurovent","(1) - Nazivni učini hlađenja se temelje na: unutarnjoj temperaturi: 27 °CDB, 19 °CWB, vanjskoj temperaturi: 35 °CDB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju visoke učinkovitosti, certifikat Eurovent","(1) - Nazivni učini hlađenja se temelje na: unutarnjoj temperaturi: 27 °CDB, 19 °CWB, vanjskoj temperaturi: 35 °CDB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju visoke učinkovitosti, certifikat Eurovent"]
["","","","","(2) - Nazivni učini grijanja temelje se na: unutarnjoj temperaturi: 20 °CDB, vanjskoj temperaturi: 7 °CDB, 6 °CWB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju standardne učinkovitosti","(2) - Nazivni učini grijanja temelje se na: unutarnjoj temperaturi: 20 °CDB, vanjskoj temperaturi: 7 °CDB, 6 °CWB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju standardne učinkovitosti","(2) - Nazivni učini grijanja temelje se na: unutarnjoj temperaturi: 20 °CDB, vanjskoj temperaturi: 7 °CDB, 6 °CWB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju standardne učinkovitosti","(2) - Nazivni učini grijanja temelje se na: unutarnjoj temperaturi: 20 °CDB, vanjskoj temperaturi: 7 °CDB, 6 °CWB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju standardne učinkovitosti"]
["","","","","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima"]