{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-F / ARXF-A"]
[]
[]
[]
[]
["","","","","ATXF50F5V1B / ARXF50A5V1B"]
["Outdoor unit","","","","ARXF50A5V1B"]
["Učin hlađenja","Min.","","kW","1.7"]
["","Nom.","","kW","5"]
["","Maks.","","kW","6"]
["Učin grijanja","Min.","","kW","1.7"]
["","Nom.","","kW","6"]
["","Maks.","","kW","7.7"]
["Nazivna učinkovitost","EER","","","3.3"]
["","COP","","","3.71"]
["","Godišnja potrošnja energije","","kWh","283"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","A"]
["","","Grijanje","","A"]
["Hlađenje prostora","Razred energetske učinkovitosti","","","A++"]
["","Kapacitet","Pdesign","kW","5"]
["","SEER","","","6.18"]
["","Godišnja potrošnja energije","","kWh/a","283"]
["Grijanje prostora (prosječna klima)","Razred energetske učinkovitosti","","","A+"]
["","Kapacitet","Pdesign","kW","4.6"]
["","SCOP/A","","","4.03"]
["","Pdh kapacitet grijanja pri -10°","","kW","4.06"]
["","Godišnja potrošnja energije","","kWh/a","1598"]
["Napomene","","","","(1) - Nazivni učini hlađenja se temelje na: unutarnjoj temperaturi: 27 °CDB, 19 °CWB, vanjskoj temperaturi: 35 °CDB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju visoke učinkovitosti, certifikat Eurovent"]
["","","","","(2) - Nazivni učini grijanja temelje se na: unutarnjoj temperaturi: 20 °CDB, vanjskoj temperaturi: 7 °CDB, 6 °CWB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju standardne učinkovitosti"]
["","","","","(3) - Vidi električne podatke na posebnim nacrtima"]