{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-F / ARXF-E"]
[]
[]
[]
[]
["","","","","ATXF20F5V1B / ARXF20E5V1B","ATXF25F5V1B / ARXF25E5V1B","ATXF35F5V1B / ARXF35E5V1B","ATXF42F5V1B / ARXF42E5V1B"]
["Outdoor unit","","","","ARXF20E5V1B","ARXF25E5V1B","ARXF35E5V1B","ARXF42E5V1B"]
["Učin hlađenja","Min.","","kW","1.3","1.3","1.3","1.4"]
["","Nom.","","kW","2","2.5","3.3","4.2"]
["","Maks.","","kW","2.4","2.8","3.8","4.3"]
["Učin grijanja","Min.","","kW","1.3","1.3","1.3","1.4"]
["","Nom.","","kW","2.4","2.8","3.5","4.6"]
["","Maks.","","kW","3.3","3.7","4.4","5"]
["Nazivna učinkovitost","EER","","","3.33","3.24","3.27","3.27"]
["","COP","","","3.75","3.73","3.72","3.71"]
["","Godišnja potrošnja energije","","kWh","109","137","191","228"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","A","A","A","A"]
["","","Grijanje","","A","A","A","A"]
["Hlađenje prostora","Razred energetske učinkovitosti","","","A++","A++","A++","A++"]
["","Kapacitet","Pdesign","kW","2","2.5","3.5","4.2"]
["","SEER","","","6.4","6.4","6.4","6.45"]
["","Godišnja potrošnja energije","","kWh/a","109","137","191","228"]
["Grijanje prostora (prosječna klima)","Razred energetske učinkovitosti","","","A+","A+","A+","A+"]
["","Kapacitet","Pdesign","kW","2.2","2.4","2.6","3.3"]
["","SCOP/A","","","4.16","4.1","4.1","4.25"]
["","Pdh kapacitet grijanja pri -10°","","kW","1.86","1.97","2.21","2.61"]
["","Godišnja potrošnja energije","","kWh/a","740","819","889","1088"]
["Napomene","","","","(1) - Nazivni učini hlađenja se temelje na: unutarnjoj temperaturi: 27 °CDB, 19 °CWB, vanjskoj temperaturi: 35 °CDB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju visoke učinkovitosti, certifikat Eurovent","(1) - Nazivni učini hlađenja se temelje na: unutarnjoj temperaturi: 27 °CDB, 19 °CWB, vanjskoj temperaturi: 35 °CDB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju visoke učinkovitosti, certifikat Eurovent","(1) - Nazivni učini hlađenja se temelje na: unutarnjoj temperaturi: 27 °CDB, 19 °CWB, vanjskoj temperaturi: 35 °CDB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju visoke učinkovitosti, certifikat Eurovent","(1) - Nazivni učini hlađenja se temelje na: unutarnjoj temperaturi: 27 °CDB, 19 °CWB, vanjskoj temperaturi: 35 °CDB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju visoke učinkovitosti, certifikat Eurovent"]
["","","","","(2) - Nazivni učini grijanja temelje se na: unutarnjoj temperaturi: 20 °CDB, vanjskoj temperaturi: 7 °CDB, 6 °CWB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju standardne učinkovitosti","(2) - Nazivni učini grijanja temelje se na: unutarnjoj temperaturi: 20 °CDB, vanjskoj temperaturi: 7 °CDB, 6 °CWB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju standardne učinkovitosti","(2) - Nazivni učini grijanja temelje se na: unutarnjoj temperaturi: 20 °CDB, vanjskoj temperaturi: 7 °CDB, 6 °CWB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju standardne učinkovitosti","(2) - Nazivni učini grijanja temelje se na: unutarnjoj temperaturi: 20 °CDB, vanjskoj temperaturi: 7 °CDB, 6 °CWB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju standardne učinkovitosti"]
["","","","","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima"]