{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-F"]
[]
[]
[]
[]
["","","","","","ATXF50F5V1B"]
["Ulazna struja","Hlađenje","","Nom.","kW","0.04"]
["","Grijanje","","Nom.","kW","0.04"]
["Kućište","Boja","","","","Bijelo"]
["Dimenzije","Uređaj","","Visina","mm","286"]
["","","","Širina","mm","770"]
["","","","Dubina","mm","225"]
["Težina","Uređaj","","","kg","9"]
["Ventilator","Količina zraka","Hlađenje","Visoko","m³/min","12.6"]
["","Protok zraka","Hlađenje","Srednji","m³/min","9"]
["","","","Nizak","m³/min","7.2"]
["","","","Tihi način rada","m³/min","6.4"]
["","","Grijanje","Visoko","m³/min","12.8"]
["","Protok zraka","Grijanje","Srednji","m³/min","9.6"]
["","","Grijanje","Nizak","m³/min","7.2"]
["","","","Tihi način rada","m³/min","6.4"]
["Zvučna snaga","Hlađenje","","","dBA","59"]
["","Grijanje","","","dBA","59"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","45"]
["Razina zvučnog tlaka","Hlađenje","","Srednji","dBA","39"]
["Razina tlaka zvuka","Hlađenje","","Nizak","dBA","34"]
["","","","Tihi način rada","dBA","31"]
["","Grijanje","","Visoko","dBA","44"]
["Razina zvučnog tlaka","Grijanje","","Srednji","dBA","38"]
["Razina tlaka zvuka","Grijanje","","Nizak","dBA","33"]
["","","","Tihi način rada","dBA","30"]
["Priključci cjevovoda","Tekućina","","VP","mm","6"]
["","Plin","","VP","mm","12.7"]
["","Odvod vode","","","","18"]
["Upravljački sustavi","Infracrveno daljinsko upravljanje","","","","ARC480A93"]
["","Žično daljinsko upravljanje","","","","BRC073A1"]
["Standardna dodatna oprema","ATXF50F5V1B","","","","1"]
["","Installation manual","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Indoor unit fixing screws","","","","2"]
["","Infrared remote control","","","","1"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Napajanje","Faza","","","","1~"]
["","Frekvencija","","","Hz","50"]
["","Napon","","","V","220-440"]
["Napomene","","","","","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 5 m; razlika razine: 0 m"]
["","","","","","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 5 m (vodoravno)"]
["","","","","","(3) - Vidi električne podatke na posebnim nacrtima"]