{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":8,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R / ARXM-R9"]
[]
[]
[]
[]
["","","","","ATXM25R2V1B / ARXM25R5V1B9","ATXM25R5V1B / ARXM25R5V1B9","ATXM35R2V1B / ARXM35R5V1B9","ATXM35R5V1B / ARXM35R5V1B9"]
["Učin hlađenja","Min.","","kW","","","1.40"]
["","Maks.","","kW","","","4.00"]
["","Nom.","","kW","","","3.40"]
["Nazivna učinkovitost","Annual energy consumption","","kWh","","","402"]
["","EER","","","","","4.23"]
["","COP","","","","","4.04"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","","","A"]
["","","Grijanje","","","","A"]
["Učin grijanja","Nom.","","kW","","","4.00"]
["","Min.","","kW","","","1.40"]
["","Maks.","","kW","","","5.20"]
["Napomene","","","","","","(1) - Pogledajte odvojene nacrte za radno područje"]
["","","","","","","(2) - Vidi električne podatke na posebnim nacrtima"]
["","","","","","","(3) - Nominalan kapacitet hlađenja se temelji se na sljedećim parametrima: unutarnja temperatura: 27 °C DB, 19 °C WB, vanjska temperatura: 35 °C DB, odgovarajuće cijevi rashladnog sredstva: 5 m, razlika u visini: 0m."]
["","","","","","","(4) - Nazivni učin grijanja zasnovani su na: unutarnja temperatura: 20°C DB, vanjska temperatura : 7°C DB, 6°C WB, odgovarajući cjevovod za radnu tvar: 5 m, razlika razine: 0 m."]
["Učin hlađenja","Min.","","kW","1.30","1.30","","1.40"]
["","Nom.","","kW","2.50","2.50","","3.40"]
["","Maks.","","kW","3.20","3.20","","4.00"]
["Učin grijanja","Min.","","kW","1.30","1.30","","1.40"]
["","Nom.","","kW","2.80","2.80","","4.00"]
["","Maks.","","kW","4.70","4.70","","5.20"]
["Nazivna učinkovitost","EER","","","4.50","4.50","","4.23"]
["","COP","","","5.00","5.00","","4.04"]
["","Godišnja potrošnja energije","","kWh","278","278","","402"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","A","A","","A"]
["","","Grijanje","","A","A","","A"]
["Hlađenje prostora","Razred energetske učinkovitosti","","","A+++","A+++","","A+++"]
["","Kapacitet","Pdesign","kW","2.50","2.50","","3.40"]
["","SEER","","","8.55","8.55","","8.55"]
["","Godišnja potrošnja energije","","kWh/a","102","102","","139"]
["Grijanje prostora (prosječna klima)","Razred energetske učinkovitosti","","","A+++","A+++","","A+++"]
["","Kapacitet","Pdesign","kW","2.40","2.40","","2.50"]
["","SCOP/A","","","5.10","5.10","","5.10"]
["","Pdh kapacitet grijanja pri -10°","","kW","2.30","2.30","","2.35"]
["","Godišnja potrošnja energije","","kWh/a","659","659","","686"]
["Raspon energetske učinkovitosti","","","","A+++ ~ D","A+++ ~ D","","A+++ ~ D"]