{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":7,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-K3 / ARXP-K3"]
[]
[]
[]
[]
["","","","","ATXP20K3V1B / ARXP20K3V1B","ATXP25K3V1B / ARXP25K3V1B","ATXP35K3V1B / ARXP35K3V1B"]
["Učin hlađenja","Nom.","","kW","2.00","2.50","3.50"]
["Nazivna učinkovitost","EER","","","3.98","3.79","3.45"]
["","COP","","","4.77","4.36","4.02"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","A","A","A"]
["","","Grijanje","","A","A","A"]
["Učin grijanja","Nom.","","kW","2.50","3.00","4.00"]
["Napomene","","","","(1) - Hlađenje: T2: unutarnja temperatura 26,6 °C DB, 19,4 °C WB, vanjska temperatura: 48°CDB [Btu/hr/W]","(1) - Hlađenje: T2: unutarnja temperatura 26,6 °C DB, 19,4 °C WB, vanjska temperatura: 48°CDB [Btu/hr/W]","(1) - Hlađenje: T2: unutarnja temperatura 26,6 °C DB, 19,4 °C WB, vanjska temperatura: 48°CDB [Btu/hr/W]"]
["","","","","(2) - Nazivni učin grijanja zasnovani su na: unutarnja temperatura: 20°C DB, vanjska temperatura : 7°C DB, 6°C WB, odgovarajući cjevovod za radnu tvar: 5 m, razlika razine: 0 m.","(2) - Nazivni učin grijanja zasnovani su na: unutarnja temperatura: 20°C DB, vanjska temperatura : 7°C DB, 6°C WB, odgovarajući cjevovod za radnu tvar: 5 m, razlika razine: 0 m.","(2) - Nazivni učin grijanja zasnovani su na: unutarnja temperatura: 20°C DB, vanjska temperatura : 7°C DB, 6°C WB, odgovarajući cjevovod za radnu tvar: 5 m, razlika razine: 0 m."]
["","","","","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima"]