{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":11,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-L"]
[]
[]
[]
[]
["","","","","","ATXP20L2V1B","ATXP20L5V1B","ATXP25L2V1B","ATXP25L5V1B","ATXP35L2V1B","ATXP35L5V1B"]
["Ulazna struja","Hlađenje","","Nom.","kW","0.017","0.017","0.019","0.019","0.032","0.032"]
["","Grijanje","","Nom.","kW","0.02","0.02","0.02","0.02","0.032","0.032"]
["Kućište","Boja","","","","Bijelo","Bijelo","Bijelo","Bijelo","Bijelo","Bijelo"]
["Dimenzije","Uređaj","","Visina","mm","286","286","286","286","286","286"]
["","","","Širina","mm","770","770","770","770","770","770"]
["","","","Dubina","mm","225","225","225","225","225","225"]
["Težina","Uređaj","","","kg","9","9","9","9","9","9"]
["Ventilator","Količina zraka","Hlađenje","Visoko","m³/min","9.8","9.8","10.1","10.1","11.5","11.5"]
["","Protok zraka","Hlađenje","Srednji","m³/min","7.9","7.9","8.1","8.1","8.3","8.3"]
["","","","Nizak","m³/min","5.9","5.9","6.1","6.1","6.3","6.3"]
["","","","Tihi način rada","m³/min","4.4","4.4","4.4","4.4","4.5","4.5"]
["","","Grijanje","Visoko","m³/min","10.3","10.3","10.3","10.3","11.5","11.5"]
["","Protok zraka","Grijanje","Srednji","m³/min","8.4","8.4","8.6","8.6","9","9"]
["","","Grijanje","Nizak","m³/min","6.5","6.5","6.7","6.7","7","7"]
["","","","Tihi način rada","m³/min","5.3","5.3","5.3","5.3","5.3","5.3"]
["Zvučna snaga","Hlađenje","","","dBA","55","55","55","55","58","58"]
["","Grijanje","","","dBA","55","55","55","55","58","58"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","39","39","40","40","43","43"]
["Razina zvučnog tlaka","Hlađenje","","Srednji","dBA","33","33","33","33","34","34"]
["Razina tlaka zvuka","Hlađenje","","Nizak","dBA","25","25","26","26","27","27"]
["","","","Tihi način rada","dBA","20","20","20","20","20","20"]
["","Grijanje","","Visoko","dBA","39","39","40","40","40","40"]
["Razina zvučnog tlaka","Grijanje","","Srednji","dBA","34","34","34","34","35","35"]
["Razina tlaka zvuka","Grijanje","","Nizak","dBA","28","28","28","28","29","29"]
["","","","Tihi način rada","dBA","21","21","21","21","21","21"]
["Priključci cjevovoda","Tekućina","","VP","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Plin","","VP","mm","9.5","9.5","9.5","9.5","9.5","9.5"]
["","Odvod vode","","","","18","18","18","18","18","18"]
["Upravljački sustavi","Infracrveno daljinsko upravljanje","","","","","","ARC480A11","ARC480A11"]
["Upravljački sustavi","Žično daljinsko upravljanje","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standardna dodatna oprema","Installation manual","","","","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2"]
["","Operation manual","","","","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1"]
["Napajanje","Faza","","","","1~","1~","1~","1~","1~","1~"]
["","Frekvencija","","","Hz","50","50","50","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Upravljački sustavi","Infracrveno daljinsko upravljanje","","","","ARC480A11","ARC480A11","","","ARC480A11","ARC480A11"]