{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":7,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-N9 / ARXP-N"]
[]
[]
[]
[]
["","","","","ATXP20N5V1B9 / ARXP20N5V1B","ATXP25N5V1B9 / ARXP25N5V1B","ATXP35N5V1B9 / ARXP35N5V1B"]
["Vanjska jedinica","","","","ARXP20N5V1B","ARXP25N5V1B","ARXP35N5V1B"]
["Učin hlađenja","Min.","","kW","1.3","1.3","1.3"]
["","Nom.","","kW","2.00","2.50","3.50"]
["","Maks.","","kW","2.6","3.0","4.0"]
["Kapacitet grijanja","Min.","","kW","1.30","1.30","1.30"]
["","Nom.","","kW","2.50","3.00","4.00"]
["","Maks.","","kW","3.50","4.00","4.80"]
["Nazivna učinkovitost","COP","","","4.77","4.36","4.02"]
["","EER","","","3.71","3.71","3.46"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","A","A","A"]
["","","Grijanje","","A","A","A"]
["Napomene","","","","(1) - Vidi električne podatke na posebnim nacrtima","(1) - Vidi električne podatke na posebnim nacrtima","(1) - Vidi električne podatke na posebnim nacrtima"]
["","","","","(2) - Nazivni učini hlađenja se temelje na: unutarnjoj temperaturi: 27 °CDB, 19 °CWB, vanjskoj temperaturi: 35 °CDB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju visoke učinkovitosti, certifikat Eurovent","(2) - Nazivni učini hlađenja se temelje na: unutarnjoj temperaturi: 27 °CDB, 19 °CWB, vanjskoj temperaturi: 35 °CDB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju visoke učinkovitosti, certifikat Eurovent","(2) - Nazivni učini hlađenja se temelje na: unutarnjoj temperaturi: 27 °CDB, 19 °CWB, vanjskoj temperaturi: 35 °CDB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju visoke učinkovitosti, certifikat Eurovent"]
["","","","","(3) - Nazivni učini grijanja temelje se na: unutarnjoj temperaturi: 20 °CDB, vanjskoj temperaturi: 7 °CDB, 6 °CWB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju standardne učinkovitosti","(3) - Nazivni učini grijanja temelje se na: unutarnjoj temperaturi: 20 °CDB, vanjskoj temperaturi: 7 °CDB, 6 °CWB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju standardne učinkovitosti","(3) - Nazivni učini grijanja temelje se na: unutarnjoj temperaturi: 20 °CDB, vanjskoj temperaturi: 7 °CDB, 6 °CWB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju standardne učinkovitosti"]