{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":8,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-N9"]
[]
[]
[]
[]
["","","","","","ATXP20N5V1B9","ATXP25N5V1B9","ATXP35N5V1B9"]
["Ulazna struja","Hlađenje","","Nom.","kW","0.019","0.020","0.032"]
["","Grijanje","","Nom.","kW","0.023","0.023","0.032"]
["Kućište","Colour","","","","Bijelo","Bijelo","Bijelo"]
["Dimenzije","Jedinica","","Visina","mm","286","286","286"]
["","","","Širina","mm","770","770","770"]
["","","","Dubina","mm","225","225","225"]
["Težina","Uređaj","","","kg","8.50","8.50","9.00"]
["Ventilator","Protok zraka","Hlađenje","Visoko","m³/min","9.5","9.7","11.5"]
["","","","Srednji","m³/min","7.4","7.7","8.3"]
["","","","Nizak","m³/min","5.6","5.8","6.3"]
["","","","Tihi način rada","m³/min","4.2","4.2","4.5"]
["","","Grijanje","Visoko","m³/min","10.4","10.4","11.5"]
["","","","Srednji","m³/min","8.1","8.1","9.0"]
["","","","Nizak","m³/min","6.2","6.4","7.0"]
["","","","Tihi način rada","m³/min","5.2","5.2","5.1"]
["Razina zvučne snage","Hlađenje","","","dBA","55","55","58"]
["","Grijanje","","","dBA","55","55","58"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","39","40","43"]
["","","","Srednji","dBA","33","33","34"]
["","","","Nizak","dBA","25","26","27"]
["","","","Tihi način rada","dBA","19","19","20"]
["","Grijanje","","Visoko","dBA","39","40","40"]
["","","","Srednji","dBA","34","34","35"]
["","","","Nizak","dBA","28","28","29"]
["","","","Tihi način rada","dBA","21","21","21"]
["Priključci cjevovoda","Tekućina","","VP","mm","6","6","6"]
["","Plin","","VP","mm","9.50","9.50","9.50"]
["","Odvod vode","","","","18","18","18"]
["Upravljački sustavi","Infrared remote control","","","","ARC480A78","ARC480A78","ARC480A78"]
["","Wired remote control","","","","BRC073A1","BRC073A1","BRC073A1"]
["Standardna dodatna oprema","Priručnik za instalaciju","","","","1","1","1"]
["","Radni priručnik","","","","1","1","1"]
["","Infracrveno daljinsko upravljanje","","","","1","1","1"]
["","AAA suhe baterije","","","","2","2","2"]
["","Držač daljinskog upravljača","","","","1","1","1"]
["","Montažna ploča","","","","1","1","1"]
["","Deodorirajući filtar od titanijevog apatita","","","","1","1","1"]
["","Srebrni filter","","","","1","1","1"]
["","Učvrsni vijak unutarnje jedinice","","","","2","2","2"]
["","Opće mjere sigurnosti","","","","1","1","1"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Frekvencija","","","Hz","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240"]
["Napomene","","","","","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 5 m; razlika razine: 0 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 5 m; razlika razine: 0 m","(1) - Hlađenje: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB; duljina odgovarajućeg cjevovoda: 5 m; razlika razine: 0 m"]
["","","","","","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 5 m (vodoravno)","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 5 m (vodoravno)","(2) - Grijanje: unutarnja temperatura 20°CDB, vanjska temperatura 7°CDB, 6°CWB, odgovarajući cjevovod za radnu tvar: 5 m (vodoravno)"]
["","","","","","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima","(3) - Vidi električne podatke na posebnim nacrtima"]