{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXS-K / ARXS-L3"]
[]
[]
[]
[]
["","","","","ATXS25K3V1B / ARXS25L3V1B","ATXS25K2V1B / ARXS25L3V1B","ATXS35K3V1B / ARXS35L3V1B","ATXS35K2V1B / ARXS35L3V1B"]
["Učin hlađenja","Min.","","kW","","","1.4"]
["","Maks.","","kW","","","4.0"]
["","Nom.","","kW","2.5 (2)","","3.5 (2)"]
["Priključci cjevovoda","Tekućina","VP","mm","6.35","","6.35"]
["","Plin","VP","mm","9.5","","9.5"]
["","Odvod vode","OD","mm","18","","18"]
["Nazivna učinkovitost","Godišnja potrošnja energije","","kWh","301","","473"]
["","EER","","","4.15 (1)","","3.70 (1)"]
["","COP","","","4.52 (1)","","4.76 (1)"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","A","","A"]
["","","Grijanje","","A","","A"]
["Kapacitet grijanja","Nom.","","kW","2.8 (2)","","4.00 (2)"]
["","Min.","","kW","1.3","","1.4"]
["","Maks.","","kW","4.7","","5.2"]
["Napomene","","","","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU"]
["","","","","(2) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja","","(2) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja"]
["","","","","(3) - 220 V","","(3) - 220 V"]
["","","","","(4) - 230 V","","(4) - 230 V"]
["","","","","(5) - 240 V","","(5) - 240 V"]
["Vanjska jedinica","","","","","ARXS25L3","","ARXS35L3"]
["Učin hlađenja","Nom.","","kW","","2.5","","3.5"]
["Učin grijanja","Nom.","","kW","","2.8","","4.00"]
["Nazivna učinkovitost","EER","","","","4.15","","3.70"]
["","COP","","","","4.52","","4.76"]
["","Godišnja potrošnja energije","","kWh","","301","","473"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","","A","","A"]
["","","Grijanje","","","A","","A"]
["Hlađenje prostora","Razred energetske učinkovitosti","","","","A++","","A++"]
["","Kapacitet","Pdesign","kW","","2.50","","3.50"]
["","SEER","","","","7.51","","7.10"]
["","Godišnja potrošnja energije","","kWh/a","","117","","173"]
["Grijanje prostora (prosječna klima)","Razred energetske učinkovitosti","","","","A++","","A++"]
["","Kapacitet","Pdesign","kW","","2.50","","3.60"]
["","SCOP/A","","","","4.68","","4.61"]
["","Godišnja potrošnja energije","","kWh/a","","747","","1094"]