{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":7,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AZQS-B(8)V1"]
[]
[]
[]
[]
["","","","","","AZQS71B2V1B","AZQS140B8V1B"]
["Dimenzije","Uređaj","","Visina","mm","770","1,430"]
["","","","Širina","mm","900","940"]
["","","","Dubina","mm","320","320"]
["Težina","Uređaj","","","kg","67","94.9"]
["Kompresor","Tip","","","","Hermetički zabrtvljen kompresor s klatnom_","Hermetički zabrtvljen kompresor s klatnom_"]
["Radno područje","Hlađenje","Ambijent:","Min.","°CDB","-5","-5.0"]
["","","","Maks.","°CDB","46","46.0"]
["","Grijanje","Ambijent:","Min.","°CWB","-15","-15.0"]
["","","","Maks.","°CWB","15.5","15.5"]
["Sound power level","Hlađenje","","","dBA","64","70.0"]
["","Grijanje","","","dBA","","70.0"]
["Razina tlaka zvuka","Hlađenje","","Nom.","dBA","48","53"]
["","Grijanje","","Nom.","dBA","50","54"]
["","Noćni tihi način rada","","Razina 1","dBA","43","49"]
["Radna tvar","Tip","","","","R-410A","R-410A"]
["","Punjenje","","","kg","2.75","4.0"]
["","GWP","","","","2,087.5","2,087.5"]
["Priključci cjevovoda","Tekućina","","VP","mm","9.52","9.52"]
["","Plin","","VP","mm","15.9","15.9"]
["","Duljina cjevovoda","Maks.","OU - IU","m","50","50, 30 (1)"]
["","","Sistem","Ekvivalent","m","70","70, 40 (1)"]
["","","","Ne puni se","m","30","30"]
["","Punjenje dodatne radne tvari","","","kg/m","Pogledajte priručnik za instalaciju","Pogledajte priručnik za instalaciju"]
["","razlika u razini","IU - OU","Maks.","m","30.0","30.0"]
["","","IU - IU","Maks.","m","","0.5"]
["Standardna dodatna oprema","Vezice","","","","2"]
["","Priručnik za instalaciju","","","","1"]
["Power supply","Faza","","","","1~","1~"]
["","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","220-240","220-240"]
["Struja - 50 Hz","Preporučeni osigurač (MFA)","","","A","","40"]
["Napomene","","","","","(1) - PED: sklop = kategorija l : isključeno iz PED opsega zbog članka 1., stavke 3.6 od 97/23/EC","(1) - Za kombinacije FCAG ~ AVEB unutarnjih jedinica"]
["","","","","","(2) - Minimalna Ssc (=Struja kratkog spoja) vrijednost: Oprema je u skladu s EN/IEC 61000-3-12: Europska/međunarodna tehnička norma koja postavlja ograničenja za harmoničke struje koje proizvodi oprema priključena na javni niskonaponski sustav s ulaznom strujom > 16 A i ≤ 75 A po fazi","(2) - EN/IEC 61000-3-12: europska/međunarodna tehnička norma koja postavlja ograničenja za harmoničke struje koje proizvode oprema priključena na javni niskonaponski sustav s ulaznom strujom većom od 16 A i ≤ 75 A po fazi"]
["","","","","","(3) - RLA je zasnovana na slijedećim uvjetima: unutarnja temperatura 27°CDB, 19°CWB; vanjska temperatura 35°CDB","(3) - Ssc: kratkospojna struja"]
["","","","","","(4) - MFA se koristi za izbor prekidača strujnog kruga i prekidača greške pri uzemljenju (prekidač propuštanja uzemljenja).","(4) - PED: sklop = kategorija l : isključeno iz PED opsega zbog članka 1., stavke 3.6 od 97/23/EC"]
["","","","","","(5) - Sadrži fluorovodične stakleničke plinove","(5) - Vidi električne podatke na posebnim nacrtima"]
["","","","","","","(6) - EN/IEC 61000-3- 11: Europska/međunarodna tehnička norma koja postavlja ograničenja za promjene napona, fluktuacije napona i titranje u javnim niskonaponskim sustavima za opremu s nazivnim strujama ≤ 75A"]