{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1HHDS"]
[]
[]
[]
[]
["","","","","BRC1HHDASA","BRC1HHDAS (Archived)"]
["Kućište","Boja","","","Srebrni","Srebrni"]
["","Poklopac gumba","","","Ne","Ne"]
["","LED lampica rada","Boja","","Plavi status indikatora","Plavi status indikatora"]
["Dimenzije","Uređaj","Visina","mm","85","85"]
["","","Širina","mm","85","85"]
["","","Dubina","mm","25","25"]
["","Pakirana jedinica","Visina","mm","50","50"]
["","","Širina","mm","217","217"]
["","","Dubina","mm","161","161"]
["Težina","Uređaj","","kg","0.110","0.110"]
["","Pakirana jedinica","","kg","0.317","0.317"]
["Pakiranje","Materijal","","","Karton","Karton"]
["","Težina","","kg","0.0850","0.0850"]
["LCD","Tip","","","100 x 150 točki","100 x 150 točki"]
["","Dimenzije","Visina","mm","40.7","40.7"]
["","","širina","mm","28.0","28.0"]
["","Pozadinsko svjetlo","Boja","","Bijelo","Bijelo"]
["Temperatura okoline","Rad","Min.","°C","-10","-10"]
["","","Maks.","°C","50","50"]
["","Pohrana","Min.","°C","-20","-20"]
["","","Maks.","°C","70","70"]
["","Temperatura okoline-=-Relativna vlažnost <-=-%","","%","95","95"]
["Upravljački sustavi","Razred kontrole temperature","","","VI","VI"]
["","Doprinos sezonskoj učinkovitosti grijanja prostora","","%","4.0","4.0"]
["Priključci ožičenja","Duljina ožičenja","Maks.","m","500","500"]