{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-AT"]
[]
[]
[]
[]
["","","","","CTXA15A2V1BT"]
["Razina tlaka zvuka","Grijanje","Visoko","dBA","39"]
["","","Srednji","dBA","32"]
["","","Tihi način rada","dBA","21"]
["","","Nizak","dBA","25"]
["","Hlađenje","Srednji","dBA","32"]
["","","Tihi način rada","dBA","21"]
["","","Nizak","dBA","25"]
["","","Visoko","dBA","39"]
["Standardna dodatna oprema","Priručnik za instalaciju","","","1"]
["","Radni priručnik","","","1"]
["","Zračni filtar","","","2"]
["","Infracrveno daljinsko upravljanje","","","1"]
["","Montažna ploča daljinskog kontrolnika","","","1"]
["","Vreća s vijcima","","","1"]
["","Poklopac vijka","","","1"]
["","AAA suhe baterije","","","2"]
["","Opće mjere sigurnosti","","","1"]
["Radna tvar","GWP","","","675.0"]
["Upravljački sustavi","Wired remote control","","","BRC073"]
["","Infrared remote control","","","ARC466A58"]
["Promjer cjevovoda","Liquid","OD","mm","6.35"]
["","Plin","OD","mm","9.50"]
["","Odvod vode","","","18"]
["Ulazna struja","Hlađenje","Nom.","kW","0.020"]
["","Grijanje","Nom.","kW","0.020"]
["Sound power level","Hlađenje","","dBA","57"]
["Dimenzije","Jedinica","Širina","mm","798"]
["","","Dubina","mm","189"]
["","","Visina","mm","295"]
["Kućište","Colour","","","Crno drvo"]
["Težina","Jedinica","","kg","12"]
["Power supply","Phase","","","1~"]
["","Frekvencija","","Hz","50"]
["","Naziv","","","V1"]
["","Napon","","V","220-240"]