{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R"]
[]
[]
[]
[]
["","","","","","CTXM15R2V1B","CTXM15R5V1B"]
["Ulazna struja","Hlađenje","","Nom.","kW","0.029","0.029"]
["","Grijanje","","Nom.","kW","0.023","0.023"]
["Kućište","Boja","","","","Bijelo","Bijelo"]
["Dimenzije","Uređaj","","Visina","mm","295","295"]
["","","","Širina","mm","778","778"]
["","","","Dubina","mm","272","272"]
["Težina","Uređaj","","","kg","10","10"]
["Ventilator","Količina zraka","Hlađenje","Visoko","m³/min","10.5","10.5"]
["","Protok zraka","Hlađenje","Srednji","m³/min","7.5","7.5"]
["","","","Nizak","m³/min","5.7","5.7"]
["","","","Tihi način rada","m³/min","4.3","4.3"]
["","","Grijanje","Visoko","m³/min","9.3","9.3"]
["","Protok zraka","Grijanje","Srednji","m³/min","8.2","8.2"]
["","","Grijanje","Nizak","m³/min","6.2","6.2"]
["","","","Tihi način rada","m³/min","5.1","5.1"]
["Zvučna snaga","Hlađenje","","","dBA","57","57"]
["","Grijanje","","","dBA","54","54"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","41","41"]
["Razina zvučnog tlaka","Hlađenje","","Srednji","dBA","33","33"]
["Razina tlaka zvuka","Hlađenje","","Nizak","dBA","25","25"]
["","","","Tihi način rada","dBA","19","19"]
["","Grijanje","","Visoko","dBA","39","39"]
["Razina zvučnog tlaka","Grijanje","","Srednji","dBA","34","34"]
["Razina tlaka zvuka","Grijanje","","Nizak","dBA","26","26"]
["","","","Tihi način rada","dBA","20","20"]
["Priključci cjevovoda","Tekućina","","VP","mm","6.35","6.35"]
["","Plin","","VP","mm","9.5","9.5"]
["","Odvod vode","","","","18","18"]
["Upravljački sustavi","Infracrveno daljinsko upravljanje","","","","ARC466A67","ARC466A67"]
["Upravljački sustavi","Žično daljinsko upravljanje","","","","BRC073A1","BRC073A1"]
["Standardna dodatna oprema","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","WLAN adapter kit","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Napajanje","Naziv","","","","V1","V1"]
["","Faza","","","","1~","1~"]
["","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","220-240","220-240"]