{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":9,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","D2U30GB-A"]
[]
[]
[]
[]
["","","","","","D2U30GB015AB","D2U30GB020AB","D2U30GB015AA (Archived)","D2U30GB020AA (Archived)"]
["Gubici topline","Kotao u pripravnosti Ps","","","kW","0.0","0.0"]
["","Kotao u pripravnosti","","","kWh/24 h","","","1.5","1.5"]
["","Kotao u pripravnosti qS","","","kW","0.0","0.0"]
["Potrošna topla voda","Početna toplina (bruto kalorična vrijednost) Qnw","Nom.","Maks.","kW","16.7","22.2","16.7","22.2"]
["","","","Min.","kW","3.3","3.3","3.3","3.3"]
["","izlaz","","Min.","kW","3.0","3.0","3.0","3.0"]
["","Temperatura","","Maks.","°C","70","70","85","85"]
["","Početna toplina (neto kalorična vrijednost) Qnw","Nom.","Min.","kW","3.0","3.0","3.0","3.0"]
["","","","Maks.","kW","15.0","20.0","15.0","20.0"]
["","Učinkovitost","","NL karakteristike (DIN4708)","","2.0","2.1","2.0","2.1"]
["Dimni plinovi","Temperatura","","Maks.","°C","63","69","63","69"]
["","Protok (G31)","","Maks.","kg/h","22.5","30.0","22.5","30.0"]
["Dobavni zrak","Koncentrično","","","","Da","Da","Da","Da"]
["Grijanje potrošne tople vode","Općenito","","Razred energetske učinkovitosti grijanja vode","","A","A","A","A"]
["","","","Deklarirani profil opterećenja","","L","L","L","L"]
["Dimenzije","Jedinica","Visina","Kućište","mm","1,895","1,895","1,895","1,895"]
["Kućište","Boja","","","","Čisto bijelo (RAL9016)/ tamno sivo (RAL7011)","Čisto bijelo (RAL9016)/ tamno sivo (RAL7011)","Čisto bijelo (RAL9016)/ tamno sivo (RAL7011)","Čisto bijelo (RAL9016)/ tamno sivo (RAL7011)"]
["Spremnik","Materijal","","","","Polipropilen","Polipropilen","Polipropilen","Polipropilen"]
["Grijanje prostora","Općenito","","Razred učinkovitosti sezonske učinkovitosti grijanja","","A","A","A","A"]
["","","","ηs (Sezonska učinkovitost grijanja prostora)","%","91","92","91","92"]
["Centralno grijanje","Početna toplina Qn (bruto kalorična vrijednost)","Nom.","Min.","kW","3.3","3.3","3.3","3.3"]
["","","","Maks.","kW","16.7","22.2","16.7","22.2"]
["","Temperatura vode","","Maks.","°C","85","85","90","90"]
["","Priključna Pm pri 80/60°C","","Min.","kW","2.9","2.9","2.9","2.9"]
["","","","Nom.","kW","14.6","19.5","14.6","19.5"]
["","Početna toplina Qn (neto kalorična vrijednost)","Nom.","Maks.","kW","15.0","20.0","15.0","20.0"]
["","","","Min.","kW","3.0","3.0","3.0","3.0"]
["","Priključna Pnc pri 50/30°C","","Min.","kW","3.2","3.2","3.2","3.2"]
["","","","Nom.","kW","15.7","20.9","15.7","20.9"]
["Plin","Priključak","","Presjek","mm","20","20","20","20"]
["","Potrošnja (G31)","","Min.","m³/h","0.16","0.16","0.16","0.16"]
["","","","Maks.","m³/h","0.62","0.82","0.62","0.82"]
["","NOx razred","","","","6","6","6","6"]
["Napomene","","","","","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897"]