{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCS601C51"]
[]
[]
[]
[]
["","","","","","DCS601C51."]
["Ulaz","Tip","","","","Dodirni zaslon (10 bitni kodirani analogni ulaz)"]
["Temperatura okoline","Relativna vlažnost <","","","%","85"]
["","Rad","","Min.","°C","0"]
["","","","Maks.","°C","40"]
["Maksimalni broj spojivih unutarnjih jedinica","","","","","64, 128 (1)"]
["Komunikacija","DIII-NET","","Količina","","1"]
["","","","Primjedba","","Komunikacijski vod klimatizacijske opreme"]
["","10BASE-T","","Primjedba","","Web opcija"]
["","Ethernet","","Primjedba","","Ulaz za internetski pristup i funkciju e-pošte"]
["","Ulazni terminal","Digitalni","Količina","","1"]
["","","","Primjedba","","Obvezno isključivanje"]
["","","Puls","Količina","","3"]
["","","","Primjedba","","Puls mjerenja napajanja"]
["","Modem","","Primjedba","","Mogućnost integracije modema"]
["","PCMCIA","","Primjedba","","Flash memorijska kartica"]
["","RS-232C","","Primjedba","","DIII-NET PLUS adapter"]
["Dimenzije","Uređaj","","Širina","mm","230"]
["","","","Depth","mm","107"]
["","","","Visina","mm","147"]
["LCD","Tip","","","","QVGA (320 x 240), 4.096 boja"]
["","Dimenzije","","Širina","cola","5.7"]
["Maksimalni broj spojivih vanjskih jedinica","","","","","10, 20 (1)"]
["Power supply","Frekvencija","","","Hz","50/60"]
["","Napon","","","V","100-240 (vanjsko napajanje)"]
["Napomene","","","","","(1) - Kombinirano s DCS601A51"]