{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":9,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSXB-D / ERLA-DW17"]
[]
[]
[]
[]
["","","","","","EBSXB16P30DF / ERLA16D2W17","EBSXB16P50DF / ERLA16D2W17","EBSXB16P30DF / ERLA16DAW17","EBSXB16P50DF / ERLA16DAW17"]
["Indoor unit","","","","","EBSXB16P30DF","EBSXB16P50DF","EBSXB16P30DF","EBSXB16P50DF"]
["Učin grijanja","Nom.","","","kW","16.0 (1)","16.0 (1)","16.0 (1)","16.0 (1)"]
["Učin hlađenja","Nom.","","","kW","13.6 (2)","13.6 (2)","13.6 (2)","13.6 (2)"]
["Ulazna struja","Grijanje","","Nom.","kW","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)"]
["","Hlađenje","","Nom.","kW","4.68 (2)","4.68 (2)","4.68 (2)","4.68 (2)"]
["COP","","","","","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)"]
["EER","","","","","2.91 (2)","2.91 (2)","2.91 (2)","2.91 (2)"]
["Grijanje potrošne tople vode","Općenito","","Deklarirani profil opterećenja","","L","XL","L","XL"]
["","Prosječni klimatski uvjeti","","Razred energetske učinkovitosti grijanja vode","","A+","A+","A+","A+"]
["Grijanje prostora","Izlaz za vodu u prosječnoj klimi 55°C","Općenito","SCOP","","3.35","3.35","3.35","3.35"]
["","","","Razred sezonske učinkovitosti grijanja prostora","","A++","A++","A++","A++"]
["","Izlaz za vodu u prosječnoj klimi 35°C","Općenito","SCOP","","4.68","4.68","4.68","4.68"]
["","","","Razred sezonske učinkovitosti grijanja prostora","","A+++","A+++","A+++","A+++"]
["Napomene","","","","","(1) - Stanje 1: hlađenje Ta 35°C - LWE 18°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Stanje 1: hlađenje Ta 35°C - LWE 18°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Stanje 1: hlađenje Ta 35°C - LWE 18°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Stanje 1: hlađenje Ta 35°C - LWE 18°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Stanje 2: hlađenje Ta 35°C - LWE 7°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Stanje 2: hlađenje Ta 35°C - LWE 7°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Stanje 2: hlađenje Ta 35°C - LWE 7°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Stanje 2: hlađenje Ta 35°C - LWE 7°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]