{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":13,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSXB-D"]
[]
[]
[]
[]
["","","","","","EBSXB11P30DF","EBSXB11P50DF","EBSXB11P30DG","EBSXB11P50DG","EBSXB16P30DF","EBSXB16P50DF","EBSXB16P30DG","EBSXB16P50DG"]
["Kućište","Boja","","","","Bijela (RAL9016)/ crna (RAL9017)","Bijela (RAL9016)/ crna (RAL9017)","Bijela (RAL9016)/ crna (RAL9017)","Bijela (RAL9016)/ crna (RAL9017)","Bijela (RAL9016)/ crna (RAL9017)","Bijela (RAL9016)/ crna (RAL9017)","Bijela (RAL9016)/ crna (RAL9017)","Bijela (RAL9016)/ crna (RAL9017)"]
["","Materijal","","","","Polipropilen otporan na udar","Polipropilen otporan na udar","Polipropilen otporan na udar","Polipropilen otporan na udar","Polipropilen otporan na udar","Polipropilen otporan na udar","Polipropilen otporan na udar","Polipropilen otporan na udar"]
["Dimenzije","Uređaj","","Visina","mm","1,893","1,910","1,893","1,910","1,893","1,910","1,893","1,910"]
["","","","Širina","mm","594","792","594","792","594","792","594","792"]
["","","","Dubina","mm","680","817","680","817","680","817","680","817"]
["Težina","Uređaj","","","kg","94","117","94","117","94","117","94","117"]
["PED","Kategorija","","","","Kategorija II","Kategorija II","Kategorija II","Kategorija II","Kategorija II","Kategorija II","Kategorija II","Kategorija II"]
["Radna tvar","Tip","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0","675.0","675.0","675.0","675.0","675.0"]
["","Punjenje","","","kg","3.80","3.80","3.80","3.80","3.80","3.80","3.80","3.80"]
["","Punjenje","","","tCO2Eq","2.57","2.57","2.57","2.57","2.57","2.57","2.57","2.57"]
["Razina zvučne snage","Nom.","","","dBA","44.7","44.7","44.7","44.7","49.0","49.0","49.0","49.0"]
["Razina tlaka zvuka","Nom.","","","dBA","36.8","36.8","36.8","36.8","40.3","40.3","40.3","40.3"]
["Raspon rada","Grijanje","Na strani vode","Min.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Maks.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","Hlađenje","Ambijent:","Min.","°CDB","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","Na strani vode","Min.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Maks.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["Napajanje","Faza","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frekvencija","","","Hz","50","50","50","50","50","50","50","50"]
["","Napon","","","V","230","230","230","230","230","230","230","230"]
["Napomene","","","","","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897"]
["","","","","","(2) - Pogledajte sheme ograničenja rada","(2) - Pogledajte sheme ograničenja rada","(2) - Pogledajte sheme ograničenja rada","(2) - Pogledajte sheme ograničenja rada","(2) - Pogledajte sheme ograničenja rada","(2) - Pogledajte sheme ograničenja rada","(2) - Pogledajte sheme ograničenja rada","(2) - Pogledajte sheme ograničenja rada"]