{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSHB-E / ERGA-EV7"]
[]
[]
[]
[]
["","","","","","EHSHB04P30EF / ERGA04EAV37"]
["Unutarnja jedinica","","","","","EHSHB04P30EF"]
["Učin grijanja","Nom.","","","kW","4.36 (1), 4.60 (2)"]
["Ulazna struja","Grijanje","","Nom.","kW","0.830 (1), 1.26 (2)"]
["COP","","","","","5.23 (1), 3.65 (2)"]
["Grijanje potrošne tople vode","Općenito","","Deklarirani profil opterećenja","","L"]
["","Prosječni klimatski uvjeti","","Razred energetske učinkovitosti grijanja vode","","A+"]
["Grijanje prostora","Izlaz za vodu u prosječnoj klimi 55°C","Općenito","SCOP","","3.26"]
["","","","Razred sezonske učinkovitosti grijanja prostora","","A++"]
["","Izlaz za vodu u prosječnoj klimi 35°C","Općenito","SCOP","","4.88"]
["","","","Razred sezonske učinkovitosti grijanja prostora","","A+++"]
["Napomene","","","","","(1) - Stanje 1: hlađenje Ta 35°C - LWE 18°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Stanje 2: hlađenje Ta 35°C - LWE 7°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]