{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSHB-E"]
[]
[]
[]
[]
["","","","","","EHSHB04P30EF","EHSHB04P30EG","EHSHB08P30EF","EHSHB08P50EF","EHSHB08P50EG","EHSHB08P30EG"]
["Kućište","Boja","","","","Bijela (RAL9016)/ crna (RAL9017)","Bijela (RAL9016)/ crna (RAL9017)","Bijela (RAL9016)/ crna (RAL9017)","Bijela (RAL9016)/ crna (RAL9017)","Bijela (RAL9016)/ crna (RAL9017)","Bijela (RAL9016)/ crna (RAL9017)"]
["","Materijal","","","","Polipropilen otporan na udar","Polipropilen otporan na udar","Polipropilen otporan na udar","Polipropilen otporan na udar","Polipropilen otporan na udar","Polipropilen otporan na udar"]
["Dimenzije","Uređaj","","Visina","mm","1,892","1,891","1,892","1,905","1,910","1,891"]
["","","","Širina","mm","594","594","594","792","792","594"]
["","","","Dubina","mm","644","644","644","812","817","644"]
["Težina","Uređaj","","","kg","79","80.0","79","110","104","80.0"]
["PED","Kategorija","","","","Dio 4.3","Dio 4.3","Dio 4.3","Dio 4.3","Dio 4.3","Dio 4.3"]
["Radna tvar","Tip","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","GWP","","","","675","675.0","675","675","675.0","675.0"]
["","Punjenje","","","kg","1.5","1.50","1.5","1.5","1.50","1.50"]
["Razina zvučne snage","Nom.","","","dBA","39","39","39","39","39","39"]
["Raspon rada","Grijanje","Na strani vode","Min.","°C","18","18","18","18","18","18"]
["","","","Maks.","°C","65","65","65","65","65","65"]
["","Hlađenje","Ambijent:","Min.","°CDB","10","10","10","10","10","10"]
["","","Na strani vode","Min.","°C","5","5","5","5","5","5"]
["","","","Maks.","°C","22","22","22","22","22","22"]
["Napajanje","Faza","","","","1~","1~","1~","1~","1~","1~"]
["","Frekvencija","","","Hz","50","50","50","50","50","50"]
["","Napon","","","V","230","230","230","230","230","230"]
["Napomene","","","","","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897"]