{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBX-AV3 / EVLQ-CV3"]
[]
[]
[]
[]
["","","","","","EHYHBX08AAV3 / EVLQ08CAV3","EHYHBX08AFV3 / EVLQ08CAV3"]
["Grijanje potrošne tople vode","Općenito","","Deklarirani profil opterećenja","","XL"]
["","Prosječni klimatski uvjeti","","Razred energetske učinkovitosti grijanja vode","","A"]
["COP","","","","","4.45 (3), 3.42 (4)","4.45, 3.42"]
["Grijanje prostora","Izlaz za vodu u prosječnoj klimi 55°C","Općenito","Razred sezonske učinkovitosti grijanja prostora","","A++"]
["","","","ηs (sezonska učinkovitost grijanja prostora)","%","129"]
["","","","SCOP","","3.29"]
["Učin hlađenja","Nom.","","","kW","6.86 (4), 5.36 (4)"]
["","Min.","","","kW","2.50 (3), 2.50 (4)"]
["EER","","","","","3.42 (3), 2.29 (4)","3.42, 2.29"]
["Kapacitet grijanja","Nom.","","","kW","7.40 (3), 6.89 (4)"]
["","Min.","","","kW","1.80 (3), 1.80 (4)"]
["","Maks.","","","kW","10.0 (3), 9.53 (4)"]
["Priključna snaga","Hlađenje","","Nom.","kW","2.01 (3), 2.34 (4)"]
["","Grijanje","","Nom.","kW","1.66 (3), 2.01 (4)"]
["Napomene","","","","","(1) - Uvjet: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Stanje 1: hlađenje Ta 35°C - LWE 18°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Uvjet: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Stanje 2: hlađenje Ta 35°C - LWE 7°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]
["","","","","","(3) - Stanje 1: hlađenje Ta 35°C - LWE 18°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Tamb 35°C - LWE 7°C (DT=5°C), prolazi kroz kotao"]
["","","","","","(4) - Stanje 2: hlađenje Ta 35°C - LWE 7°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(4) - Tamb 35°C - LWE 18°C (DT=5°C), prolazi kroz kotao"]
["","","","","","(5) - Tamb 35°C - LWE 7°C (DT=5°C), prolazi kroz kotao","(5) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), prolazi kroz kotao"]
["","","","","","(6) - Tamb 35°C - LWE 18°C (DT=5°C), prolazi kroz kotao","(6) - DB/WB 7°C/6°C - LWC 45°C (DT=5°C), prolazi kroz kotao"]
["","","","","","(7) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), prolazi kroz kotao"]
["","","","","","(8) - DB/WB 7°C/6°C - LWC 45°C (DT=5°C), prolazi kroz kotao"]
["Učin grijanja","Min.","","","kW","","1.80, 1.80"]
["","Nom.","","","kW","","7.40, 6.89"]
["","Maks.","","","kW","","10.0, 9.53"]
["Učin hlađenja","Min.","","","kW","","2.50, 2.50"]
["","Nom.","","","kW","","6.86, 5.36"]
["Ulazna struja","Grijanje","","Nom.","kW","","1.66, 2.01"]
["","Hlađenje","","Nom.","kW","","2.01, 2.34"]
["Grijanje potrošne tople vode","Općenito","","Deklarirani profil opterećenja","","","XL"]
["","Prosječni klimatski uvjeti","","Razred energetske učinkovitosti grijanja vode","","","A"]
["Grijanje prostora","Izlaz za vodu u prosječnoj klimi 55°C","Općenito","SCOP","","","3.29"]
["","","","Razred sezonske učinkovitosti grijanja prostora","","","A++"]
["","Izlaz za vodu u prosječnoj klimi 35°C","Općenito","SCOP","","","4.28"]
["","","","Razred sezonske učinkovitosti grijanja prostora","","","A++"]
["Raspon energetske učinkovitosti","","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]