{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBX-AV3"]
[]
[]
[]
[]
["","","","","","EHYHBX08AFV3"]
["Kućište","Boja","","","","Bijelo"]
["","Materijal","","","","Lim prevučen zaštitnim slojem"]
["Dimenzije","Uređaj","","Visina","mm","902"]
["","","","Širina","mm","450"]
["","","","Dubina","mm","164"]
["Težina","Uređaj","","","kg","31.2"]
["PED","Kategorija","","","","Kategorija I"]
["Izmjenjivač topline na vodenoj strani","Brzina protoka vode","Grijanje","Maks.","l/min","23.5 (7)"]
["Razina zvučne snage","Nom.","","","dBA","42.0"]
["Raspon rada","Grijanje","Na strani vode","Min.","°C","25 (8)"]
["","","","Maks.","°C","55 (8)"]
["","Hlađenje","Ambijent:","Min.","°CDB","10 (8)"]
["","","Na strani vode","Min.","°C","5 (8)"]
["","","","Maks.","°C","22 (8)"]
["Napajanje","Naziv","","","","V3"]
["","Faza","","","","1~"]
["","Frekvencija","","","Hz","50"]
["","Napon","","","V","230"]
["Ožičenja","Za povezivanje s korisničkim sučeljem","","Količina","","2"]
["Priključci ožičenja","Za spajanje s korisničkim sučeljem","","Primjedba","","0,75 mm² do 1,25 mm² (maks. duljina 500m)"]
["Napomene","","","","","(1) - Samo za unutarnju jedinicu"]
["","","","","","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), prolazi kroz kotao"]
["","","","","","(3) - DB/WB 7°C/6°C - LWC 45°C (DT=5°C), prolazi kroz kotao"]
["","","","","","(4) - Tamb 35°C - LWE 7°C (DT=5°C), prolazi kroz kotao"]
["","","","","","(5) - Tamb 35°C - LWE 18°C (DT=5°C), prolazi kroz kotao"]
["","","","","","(6) - Min. required"]
["","","","","","(7) - Prolazi kroz kotao"]
["","","","","","(8) - Za radni raspon *HYHB* i *HYKOMB33AA, pogledajte nacrt radnog raspona"]