{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":7,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWET-BV3"]
[]
[]
[]
[]
["","","","","","EKHWET90BAV3","EKHWET120BAV3"]
["Montaža","","","","","Zid","Zid"]
["Kućište","Boja","","","","Bijelo + crno","Bijelo + crno"]
["","Materijal","","","","Lim, Akril-nitril-butadien-stiren","Lim, Akril-nitril-butadien-stiren"]
["Dimenzije","Jedinica","Visina","Spremnik","mm","1032","1283"]
["","Uređaj","","Širina","mm","510","510"]
["","","","Dubina","mm","570","570"]
["Težina","Jedinica","","Prazno","kg","43","47"]
["Spremnik","Volumen vode","","","l","89","118"]
["","Materijal","","","","Emajlirani čelik acc. DIN4753TL2","Emajlirani čelik acc. DIN4753TL2"]
["","Maksimalna temperatura vode","","","°C","75.0","75.0"]
["","Razred energetske učinkovitosti","","","","B","C"]
["Izmjenjivač topline","Topla voda","","Količina","","1","1"]
["","","","Materijal cijevi","","Aluminij","Aluminij"]
["","","","Radni tlak","šipka","42","42"]
["El. grijač","Učin","","","kW","1.2","1.2"]