{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":8,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWS-BA3V3"]
[]
[]
[]
[]
["","","","","","EKHWS150BA3V3","EKHWS200BA3V3","EKHWS300BA3V3"]
["Dodatni grijač","Učin","","","kW","3","3","3"]
["Dimenzije","Uređaj","","Širina","mm","595","595","595"]
["","","Visina","Spremnik","mm","945","1,195","1,645"]
["","","","Dubina","mm","595","595","595"]
["Kućište","Materijal","","","","Epoksidom presvučen meki čelik","Epoksidom presvučen meki čelik","Epoksidom presvučen meki čelik"]
["","Boja","","","","Neutralno bijela","Neutralno bijela","Neutralno bijela"]
["Spremnik","Razred energetske učinkovitosti","","","","C","C","C"]
["","Materijal","","","","Nehrđajući čelik (DIN 1.4521)","Nehrđajući čelik (DIN 1.4521)","Nehrđajući čelik (DIN 1.4521)"]
["","Volumen vode","","","l","150","200","285"]
["Težina","Jedinica","","Prazno","kg","42","49","62"]
["Napomene","","","","","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897"]