{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":10,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWS-D3V3"]
[]
[]
[]
[]
["","","","","","EKHWS150D3V3","EKHWS180D3V3","EKHWS200D3V3","EKHWS250D3V3","EKHWS300D3V3"]
["Kućište","Boja","","","","Neutralno bijela","Neutralno bijela","Neutralno bijela","Neutralno bijela","Neutralno bijela"]
["","Materijal","","","","Čelik prevučen epoksidom, Epoksidom presvučen meki čelik","Čelik prevučen epoksidom, Epoksidom presvučen meki čelik","Čelik prevučen epoksidom, Epoksidom presvučen meki čelik","Čelik prevučen epoksidom, Epoksidom presvučen meki čelik","Čelik prevučen epoksidom, Epoksidom presvučen meki čelik"]
["Dimenzije","Jedinica","Visina","Spremnik","mm","1,000","1,164","1,264","1,535","1,745"]
["","","","Presjek","mm","595","595","595","595","595"]
["Težina","Jedinica","","Prazno","kg","45","50","53","58","63"]
["","","","Puno","kg","190","224","245","300","355"]
["Spremnik","Volumen vode","","","l","145","174","192","242","292"]
["","Materijal","","","","Nehrđajući čelik (EN 1.4521)","Nehrđajući čelik (EN 1.4521)","Nehrđajući čelik (EN 1.4521)","Nehrđajući čelik (EN 1.4521)","Nehrđajući čelik (EN 1.4521)"]
["","Maksimalna temperatura vode","","","°C","75","75","75","75","75"]
["","Razred energetske učinkovitosti","","","","B","B","B","B","B"]
["Izmjenjivač topline","Topla voda","","Količina","","1","1","1","1","1"]
["","","","Materijal cijevi","","Nehrđajući čelik (EN 1.4521)","Nehrđajući čelik (EN 1.4521)","Nehrđajući čelik (EN 1.4521)","Nehrđajući čelik (EN 1.4521)","Nehrđajući čelik (EN 1.4521)"]
["","","","Volumen unutarnjih zavojnica","l","4.9","6.5","8.2","8.2","8.2"]
["","","","Radni tlak","šipka","10","10","10","10","10"]
["Dodatni grijač","Učin","","","kW","3","3","3","3","3"]
["Napomene","","","","","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897"]