{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":8,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPRA014-018DV"]
[]
[]
[]
[]
["","","","","","EPRA14DAV3","EPRA16DAV3","EPRA18DAV3"]
["Dimenzije","Uređaj","","Visina","mm","1003","1003","1003"]
["","","","Širina","mm","1270","1270","1270"]
["","","","Dubina","mm","533","533","533"]
["Težina","Uređaj","","","kg","146","146","146"]
["Radno područje","Hlađenje","","Min.","°CDB","10","10","10"]
["","","","Maksimalno","°CDB","43","43","43"]
["Raspon rada","Topla voda","","Min.","°CDB","-28","-28","-28"]
["Radno područje","Topla voda za kućanstvo","","Maksimalno","°CDB","35","35","35"]
["Razina zvučne snage","Grijanje","","Nom.","dBA","56.0","56.0","59.0"]
["","Hlađenje","","Nom.","dBA","56.0","56.0","59.0"]
["Razina tlaka zvuka","Grijanje","","Nom.","dBA","43.0","43.0","48.0"]
["","Hlađenje","","Nom.","dBA","43","43","48"]
["Radna tvar","Tip","","","","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0"]
["","Punjenje","","","tCO2Eq","2.84","2.84","2.84"]
["","Punjenje","","","kg","4.2","4.2","4.2"]
["Priključci cjevovoda","Razlika razine","IU - OU","Maks.","m","10.0","10.0","10.0"]
["Napajanje","Naziv","","","","V3","V3","V3"]
["","Faza","","","","1~","1~","1~"]
["","Frekvencija","","","Hz","50","50","50"]
["","Napon","","","V","230","230","230"]
["Struja","Preporučeni osigurači","","","A","32","32","32"]
["Napomene","","","","","(1) - hlađenje Ta 35 °C - LWE 18°C ( DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C ( DT = 5°C )","(1) - hlađenje Ta 35 °C - LWE 18°C ( DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C ( DT = 5°C )","(1) - hlađenje Ta 35 °C - LWE 18°C ( DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C ( DT = 5°C )"]
["","","","","","(2) - Razina zvučnog tlaka mjeri se mikro. na propisanoj udaljenosti od jedinice. To je relativna vrijednost koja ovisi o udaljenosti i zvučnom okruženju. Više info. potražite na crtežu sa zvučnim spektrom. Uvjeti: Ta DB/WB(temp.suhog termometra/temp. mokrog termometra), 6°CWB 7°C/6°C-LWC 35°C(DT=5°C).","(2) - Razina zvučnog tlaka mjeri se mikro. na propisanoj udaljenosti od jedinice. To je relativna vrijednost koja ovisi o udaljenosti i zvučnom okruženju. Više info. potražite na crtežu sa zvučnim spektrom. Uvjeti: Ta DB/WB(temp.suhog termometra/temp. mokrog termometra), 6°CWB 7°C/6°C-LWC 35°C(DT=5°C).","(2) - Razina zvučnog tlaka mjeri se mikro. na propisanoj udaljenosti od jedinice. To je relativna vrijednost koja ovisi o udaljenosti i zvučnom okruženju. Više info. potražite na crtežu sa zvučnim spektrom. Uvjeti: Ta DB/WB(temp.suhog termometra/temp. mokrog termometra), 6°CWB 7°C/6°C-LWC 35°C(DT=5°C)."]
["","","","","","(3) - Postotak učina grijanja pri Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Postotak učina grijanja pri Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Postotak učina grijanja pri Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]