{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERGA-EVH7"]
[]
[]
[]
[]
["","","","","","ERGA08EAV3H7"]
["Dimenzije","Uređaj","","Visina","mm","740"]
["","","","Širina","mm","884"]
["","","","Dubina","mm","388"]
["Težina","Uređaj","","","kg","58.5"]
["Radno područje","Hlađenje","","Min.","°CDB","10"]
["","","","Maksimalno","°CDB","43"]
["Raspon rada","Topla voda","","Min.","°CDB","-25"]
["Radno područje","Topla voda za kućanstvo","","Maksimalno","°CDB","35"]
["Razina zvučne snage","Grijanje","","Nom.","dBA","62 (1)"]
["","Hlađenje","","Nom.","dBA","62 (1)"]
["Razina tlaka zvuka","Grijanje","","Nom.","dBA","49 (1)"]
["","Hlađenje","","Nom.","dBA","50 (1)"]
["Radna tvar","Tip","","","","R-32"]
["","GWP","","","","675.0"]
["","Punjenje","","","tCO2Eq","1.01"]
["","Punjenje","","","kg","1.50"]
["Priključci cjevovoda","Tekućina","","VP","mm","6"]
["","Plin","","VP","mm","15.9"]
["","Odvod vode","","OD","mm","18"]
["","Razlika razine","IU - OU","Maks.","m","30.0"]
["","Toplinska izolacija","","","","Cijevi za tekućinu i plin"]
["Napajanje","Naziv","","","","V3"]
["","Faza","","","","1N~"]
["","Frekvencija","","","Hz","50"]
["","Napon","","","V","230"]
["Struja","Preporučeni osigurači","","","A","25"]
["Napomene","","","","","(1) - hlađenje Ta 35 °C - LWE 18°C ( DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C ( DT = 5°C )"]