{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERRQ-AY1"]
[]
[]
[]
[]
["","","","","","ERRQ011AAY1","ERRQ014AAY1","ERRQ016AAY1"]
["Razina tlaka zvuka","Grijanje","","Nom.","dBA","52","53","55"]
["Standardna dodatna oprema","Priručnik za instalaciju","","","","1","1","1"]
["Razina zvučne snage","Grijanje","","Nom.","dBA","68","69","71"]
["Radna tvar","Charge","","","TCO2Eq","9.4","9.4","9.4"]
["","GWP","","","","2,087.5","2,087.5","2,087.5"]
["","Punjenje","","","kg","4.5","4.5","4.5"]
["","Tip","","","","R-410A","R-410A","R-410A"]
["Dimenzije","Uređaj","","Širina","mm","900","900","900"]
["","","","Dubina","mm","320","320","320"]
["","","","Visina","mm","1,345","1,345","1,345"]
["Radno područje","Grijanje","","Max.","°CWB","20","20","20"]
["","","","Min.","°CWB","-20","-20","-20"]
["","Topla voda","","Min.","°CDB","-20","-20","-20"]
["","","","Maksimalno","°CDB","35","35","35"]
["Težina","Uređaj","","","kg","120","120","120"]
["Priključci cjevovoda","Toplinska izolacija","","","","Cijevi za tekućinu i plin","Cijevi za tekućinu i plin","Cijevi za tekućinu i plin"]
["","Tekućina","","VP","mm","9.52","9.52","9.52"]
["","Plin","","VP","mm","15.9","15.9","15.9"]
["","Odvod vode","","OD","mm","26x3","26x3","26x3"]
["","razlika u razini","IU - OU","Maks.","m","30","30","30"]
["Power supply","Faza","","","","3~","3~","3~"]
["","Frekvencija","","","Hz","50","50","50"]
["","Naziv","","","","Y1","Y1","Y1"]
["","Napon","","","V","380-415","380-415","380-415"]
["Struja","Preporučeni osigurači","","","A","16","16","16"]
["Napomene","","","","","(1) - Pogledajte odvojene nacrte za radno područje","(1) - Pogledajte odvojene nacrte za radno područje","(1) - Pogledajte odvojene nacrte za radno područje"]
["","","","","","(2) - Sadrži fluorovodične stakleničke plinove","(2) - Sadrži fluorovodične stakleničke plinove","(2) - Sadrži fluorovodične stakleničke plinove"]