{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSH-D"]
[]
[]
[]
[]
["","","","","","ETSH16P50DA","ETSH16P30DA"]
["Razina zvučnog tlaka","Nom.","","","dBA","32.8","32.8"]
["Radno područje","Hlađenje","Ambijent:","Min.","°CDB","10","10"]
["","","Na strani vode","Maks.","°C","22","22"]
["","","","Min.","°C","5","5"]
["","Heating","Na strani vode","Maks.","°C","70","70"]
["","","","Min.","°C","15","15"]
["Razina zvučne snage","Nom.","","","dBA","45.6","45.6"]
["Dimenzije","Uređaj","","Širina","mm","785","590"]
["","","","Dubina","mm","785","615"]
["","","","Visina","mm","1,896","1,891"]
["Kućište","Materijal","","","","Polipropilen otporan na udar","Polipropilen otporan na udar"]
["","Colour","","","","Čisto bijelo (RAL9016)/ tamno sivo (RAL7011)","Čisto bijelo (RAL9016)/ tamno sivo (RAL7011)"]
["PED","Kategorija","","","","Dio 4.3","Dio 4.3"]
["Težina","Uređaj","","","kg","90","73"]
["Power supply","Phase","","","","1~","1~"]
["","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","230","230"]
["Električni grijač","Napajanje","","Frekvencija","Hz","50","50"]
["","","","Ime","","3V / 9W","3V / 9W"]
["","","","Faza","","1~ / 3~","1~ / 3~"]
["Napomene","","","","","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]