{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":17,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSHB12E / EPRA08-12EV"]
[]
[]
[]
[]
["","","","","","ETSHB12P30EF / EPRA08EAV3","ETSHB12P50EF / EPRA08EAV3","ETSHB12P30EG / EPRA08EAV3","ETSHB12P50EG / EPRA08EAV3","ETSHB12P30EF / EPRA10EAV3","ETSHB12P50EF / EPRA10EAV3","ETSHB12P30EG / EPRA10EAV3","ETSHB12P50EG / EPRA10EAV3","ETSHB12P30EF / EPRA12EAV3","ETSHB12P50EF / EPRA12EAV3","ETSHB12P30EG / EPRA12EAV3","ETSHB12P50EG / EPRA12EAV3"]
["Indoor unit","","","","","ETSHB12P30EF","ETSHB12P50EF","ETSHB12P30EG","ETSHB12P50EG","ETSHB12P30EF","ETSHB12P50EF","ETSHB12P30EG","ETSHB12P50EG","ETSHB12P30EF","ETSHB12P50EF","ETSHB12P30EG","ETSHB12P50EG"]
["Učin grijanja","Nom.","","","kW","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)"]
["Ulazna struja","Grijanje","","Nom.","kW","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)"]
["COP","","","","","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)"]
["Grijanje potrošne tople vode","Općenito","","Deklarirani profil opterećenja","","L","XL","L","XL","L","XL","L","XL","L","XL","L","XL"]
["","Prosječni klimatski uvjeti","","Razred energetske učinkovitosti grijanja vode","","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+"]
["Grijanje prostora","Izlaz za vodu u prosječnoj klimi 55°C","Općenito","SCOP","","3.41","3.41","3.41","3.41","3.43","3.43","3.43","3.43","3.43","3.43","3.43","3.43"]
["","","","Razred sezonske učinkovitosti grijanja prostora","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Izlaz za vodu u prosječnoj klimi 35°C","Općenito","SCOP","","4.69","4.69","4.69","4.69","4.71","4.71","4.71","4.71","4.71","4.71","4.71","4.71"]
["","","","Razred sezonske učinkovitosti grijanja prostora","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Raspon energetske učinkovitosti","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Napomene","","","","","(1) - Stanje 1: hlađenje Ta 35°C - LWE 18°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Stanje 1: hlađenje Ta 35°C - LWE 18°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Stanje 1: hlađenje Ta 35°C - LWE 18°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Stanje 1: hlađenje Ta 35°C - LWE 18°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Stanje 1: hlađenje Ta 35°C - LWE 18°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Stanje 1: hlađenje Ta 35°C - LWE 18°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Stanje 1: hlađenje Ta 35°C - LWE 18°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Stanje 1: hlađenje Ta 35°C - LWE 18°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Stanje 1: hlađenje Ta 35°C - LWE 18°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Stanje 1: hlađenje Ta 35°C - LWE 18°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Stanje 1: hlađenje Ta 35°C - LWE 18°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Stanje 1: hlađenje Ta 35°C - LWE 18°C (DT = 5°C); grijanje Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Uvjet: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Uvjet: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Uvjet: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Uvjet: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Uvjet: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Uvjet: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Uvjet: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Uvjet: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Uvjet: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Uvjet: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Uvjet: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Uvjet: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), s pumpom na punoj brzini","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), s pumpom na punoj brzini","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), s pumpom na punoj brzini","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), s pumpom na punoj brzini","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), s pumpom na punoj brzini","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), s pumpom na punoj brzini","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), s pumpom na punoj brzini","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), s pumpom na punoj brzini","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), s pumpom na punoj brzini","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), s pumpom na punoj brzini","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), s pumpom na punoj brzini","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), s pumpom na punoj brzini"]