{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSXB16E7"]
[]
[]
[]
[]
["","","","","","ETSXB16P30EF7","ETSXB16P30EG7","ETSXB16P50EF7","ETSXB16P50EG7"]
["Kućište","Boja","","","","Bijela (RAL9016)/ crna (RAL9017)","Bijela (RAL9016)/ crna (RAL9017)","Bijela (RAL9016)/ crna (RAL9017)","Bijela (RAL9016)/ crna (RAL9017)"]
["","Materijal","","","","Polipropilen otporan na udar","Polipropilen otporan na udar","Polipropilen otporan na udar","Polipropilen otporan na udar"]
["Dimenzije","Uređaj","","Visina","mm","1892","1892","1910","1910"]
["","","","Širina","mm","594","594","792","792"]
["","","","Dubina","mm","644","644","816","817"]
["Težina","Uređaj","","","kg","76","76","100","100"]
["Razina zvučne snage","Nom.","","","dBA","45.6","45.6","45.6","45.6"]
["Razina tlaka zvuka","Nom.","","","dBA","32.8","32.8","32.8","32.8"]
["Raspon rada","Grijanje","Na strani vode","Min.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Maks.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["","Hlađenje","Ambijent:","Min.","°CDB","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","Na strani vode","Min.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Maks.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["Napajanje","Faza","","","","1~","1~","1~","1~"]
["","Frekvencija","","","Hz","50","50","50","50"]
["","Napon","","","V","230","230","230","230"]
["Napomene","","","","","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897","(1) - Gubitak topline u skladu s EN12897"]
["","","","","","(2) - Pogledajte sheme ograničenja rada","(2) - Pogledajte sheme ograničenja rada","(2) - Pogledajte sheme ograničenja rada","(2) - Pogledajte sheme ograničenja rada"]