{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EVLQ-CV3"]
[]
[]
[]
[]
["","","","","","EVLQ05CAV3","EVLQ08CAV3"]
["Dimenzije","Uređaj","","Visina","mm","735","735"]
["","","","Širina","mm","832","832"]
["","","","Dubina","mm","307","307"]
["Težina","Uređaj","","","kg","54","56"]
["Ventilator","Količina zraka","Grijanje","Visoko","m³/min","45.0","47.0"]
["","","Hlađenje","Visoko","m³/min","525","525"]
["Raspon rada","Grijanje","","Min.","°CWB","-25","-25"]
["","","","Maks.","°CWB","25","25"]
["Razina zvučne snage","Grijanje","","Nom.","dBA","61","62"]
["Razina tlaka zvuka","Grijanje","","Nom.","dBA","48 (1)","49 (1)"]
["Radna tvar","Tip","","","","R-410A","R-410A"]
["","GWP","","","","2088","2088"]
["","Punjenje","","","tCO2Eq","3.0","3.3"]
["","Punjenje","","","kg","1.5","1.6"]
["Priključci cjevovoda","Tekućina","","VP","mm","6.35","6.35"]
["","Plin","","VP","mm","159","159"]
["","Odvod vode","","OD","mm","1x ø15 + 1x ø20","1x ø15 + 1x ø20"]
["","Razlika razine","IU - OU","Maks.","m","20.0","20.0"]
["Napajanje","Naziv","","","","V3","V3"]
["","Faza","","","","1~","1~"]
["","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","230","230"]
["Struja","Preporučeni osigurači","","","A","16","20"]
["Napomene","","","","","(1) - Razina tlaka zvuka mjeri se mikrofonom na određenoj udaljenosti od jedinice. To je relativna vrijednost, ovisna o udaljenosti i akustici okoliša. Pogledajte dijagram zvučnog spektra za više informacija.","(1) - Razina tlaka zvuka mjeri se mikrofonom na određenoj udaljenosti od jedinice. To je relativna vrijednost, ovisna o udaljenosti i akustici okoliša. Pogledajte dijagram zvučnog spektra za više informacija."]
["","","","","","(2) - Standardna uklj./isklj. struja pokretanja kompresora >> maks. radna struja","(2) - Standardna uklj./isklj. struja pokretanja kompresora >> maks. radna struja"]
["","","","","","(3) - Struja pokretanja Daikin Altherma inverterski kontroliranog kompresora uvijek je <= maks. radna struja","(3) - Struja pokretanja Daikin Altherma inverterski kontroliranog kompresora uvijek je <= maks. radna struja"]