{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWAA-DW1P-H"]
[]
[]
[]
[]
["","","","","","EWAA011DAW1P-H-","EWAA014DAW1P-H-","EWAA016DAW1P-H-"]
["Nivo zvučnog tlaka","Hlađenje","","Nom.","dBA","47.7","50.8","51.0"]
["Hidrauličke komponente","Ekspanzijska posuda","","Volumen","l","8","8","8"]
["Raspon rada","Na strani zraka","Hlađenje","Min.","°CDB","10","10","10"]
["","","","Maks.","°CDB","43","43","43"]
["","Na strani vode","Hlađenje","Maks.","°CDB","22","22","22"]
["","","","Min.","°CDB","5","5","5"]
["Količina radne tvari","Po krugu","","","kg","3.80","3.80","3.80"]
["","Refrigerant charge-=-Per circuit-=-TCO2Eq","","","TCO2Eq","2.6","2.6","2.6"]
["Kompresor","Tip","","","","Hermetički zabrtvljen inverterski kompresor s klatnom","Hermetički zabrtvljen inverterski kompresor s klatnom","Hermetički zabrtvljen inverterski kompresor s klatnom"]
["","Početna metoda_","","","","Pogonjen inverterom","Pogonjen inverterom","Pogonjen inverterom"]
["","Količina_","","","","1","1","1"]
["Zračni izmjenjivač topline","Tip","","","","Visoko učinkovita lamela i cijev s integriranim podhladnjakom","Visoko učinkovita lamela i cijev s integriranim podhladnjakom","Visoko učinkovita lamela i cijev s integriranim podhladnjakom"]
["Težina","Uređaj","","","kg","147","147","147"]
["EER","","","","","3.26 (1), 5.31 (2)","3.16 (1), 5.04 (2)","3.06 (1), 4.74 (2)"]
["Radna tvar","GWP","","","","675.0","675.0","675.0"]
["","Tip","","","","R-32","R-32","R-32"]
["","Krugovi","","Količina","","1","1","1"]
["","Upravljanje","","","","Elektronički ekspanzijski ventil","Elektronički ekspanzijski ventil","Elektronički ekspanzijski ventil"]
["Motor ventilatora","Brzina","Hlađenje","Nom.","o/min","550","650","650"]
["Učin hlađenja","Nom.","","","kW","11.6 (1), 11.5 (2)","12.8 (1), 12.7 (2)","14.0 (1), 15.3 (2)"]
["Izmjenjivač topline vode","Volumen vode","","","l","2","2","2"]
["","Min. volumen vode u sustavu","","","l","20 (6)","20 (6)","20 (6)"]
["","Tip","","","","Pločasti izmjenjivač topline","Pločasti izmjenjivač topline","Pločasti izmjenjivač topline"]
["Power input","Hlađenje","","Nom.","kW","3.56 (1), 2.17 (2)","4.06 (1), 2.51 (2)","4.58 (1), 3.24 (2)"]
["Sound power level","Hlađenje","","Nom.","dBA","67.0","69.0","69.0"]
["Dimenzije","Uređaj","","Širina","mm","1,380","1,380","1,380"]
["","","","Dubina","mm","460","460","460"]
["","","","Visina","mm","870","870","870"]
["Regulacija učina","Metoda","","","","Varijabilno (inverter)","Varijabilno (inverter)","Varijabilno (inverter)"]
["Ventilator","Količina zraka","Hlađenje","Nom.","m³/min","70","85","85"]
["Kompresor","Početna metoda_","","","","Inverter","Inverter","Inverter"]
["Power supply","Faza","","","","3~","3~","3~"]
["","Frekvencija","","","Hz","50","50","50"]
["","Naziv","","","","W1","W1","W1"]
["","Napon","","","V","400","400","400"]
["Napomene","","","","","(1) - Hlađenje: EW 12°C; LW 7°C; uvjeti okoline: 35°CDB","(1) - Hlađenje: EW 12°C; LW 7°C; uvjeti okoline: 35°CDB","(1) - Hlađenje: EW 12°C; LW 7°C; uvjeti okoline: 35°CDB"]
["","","","","","(2) - Hlađenje: EW 23°C; LW 18°C; uvjeti okoline: 35°CDB","(2) - Hlađenje: EW 23°C; LW 18°C; uvjeti okoline: 35°CDB","(2) - Hlađenje: EW 23°C; LW 18°C; uvjeti okoline: 35°CDB"]
["","","","","","(3) - Uvjet: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Uvjet: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Uvjet: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(4) - Uvjet: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(4) - Uvjet: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(4) - Uvjet: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]
["","","","","","(5) - U skladu s EN14825","(5) - U skladu s EN14825","(5) - U skladu s EN14825"]
["","","","","","(6) - Ovisi o načinu rada, pogledajte priručnik za instalaciju.","(6) - Ovisi o načinu rada, pogledajte priručnik za instalaciju.","(6) - Ovisi o načinu rada, pogledajte priručnik za instalaciju."]
["","","","","","(7) - Za više detalja pogledajte nacrt radnog raspona","(7) - Za više detalja pogledajte nacrt radnog raspona","(7) - Za više detalja pogledajte nacrt radnog raspona"]