{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":9,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FAA71BUV1B / FAA71BUV1B / RZQG100L8Y1B","FAA71BUV1B / FAA71BUV1B / RZQG125L8Y1B","FAA100BUV1B / RZQG100L8Y1B","FAA71BUV1B / RZQG71L8Y1B","FAA100BUV1B / RZQG71L8Y1B"]
["Učin hlađenja","Nom.","","kW","","","","6.80","6.80"]
["Hlađenje prostora","SEER","","","","","","6.43","6.43"]
["","Godišnja potrošnja energije","","kWh/a","","","","371","371"]
["","Kapacitet","Pdesign","kW","","","","6.80","6.80"]
["","Razred energetske učinkovitosti","","","","","","A++","A++"]
["Grijanje prostora (prosječna klima)","Kapacitet","Pdesign","kW","","","","6.33","6.33"]
["","SCOP/A","","","","","","4.02","4.02"]
["","Razred energetske učinkovitosti","","","","","","A+","A+"]
["","Godišnja potrošnja energije","","kWh/a","","","","2,205","2,205"]
["Nazivna učinkovitost","EER","","","","","","3.40","3.40"]
["","Godišnja potrošnja energije","","kWh","","","","1,000"]
["","COP","","","","","","3.70"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","","","","A"]
["","","Grijanje","","","","","A"]
["Učin grijanja","Nom.","","kW","","","","7.50"]
["Raspon energetske učinkovitosti","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Napomene","","","","","","","(1) - Nom. kapacitet hlađenja se temelji se na sljedećim parametrima: unutarnja temperatura: 27 °C DB, 19 °C WB, vanjska temperatura: 35 °C DB, odgovarajuće cijevi rashladnog sredstva: 5 m, razlika u visini: 0m.","(1) - Pogledajte odvojene nacrte za radno područje"]
["","","","","","","","(2) - Nazivni učin grijanja zasnovani su na: unutarnja temperatura: 20°C DB, vanjska temperatura : 7°C DB, 6°C WB, odgovarajući cjevovod za radnu tvar: 5 m, razlika razine: 0 m.","(2) - Vidi električne podatke na posebnim nacrtima"]
["","","","","","","","(3) - Pogledajte odvojene nacrte za radno područje"]
["","","","","","","","(4) - Vidi električne podatke na posebnim nacrtima"]