{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FAQ100CVEB / RZQSG100L8Y1B"]
["Učin hlađenja","Nom.","","kW","9.5"]
["Hlađenje prostora","SEER","","","5.61"]
["","Godišnja potrošnja energije","","kWh/a","593"]
["","Kapacitet","Pdesign","kW","9.5"]
["","Razred energetske učinkovitosti","","","A+"]
["Grijanje prostora (prosječna klima)","Kapacitet","Pdesign","kW","6.81"]
["","SCOP/A","","","4.01"]
["","Razred energetske učinkovitosti","","","A+"]
["","Godišnja potrošnja energije","","kWh/a","2,378"]
["Nazivna učinkovitost","Godišnja potrošnja energije","","kWh","1,580"]
["","EER","","","3.01"]
["","COP","","","3.41"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","B"]
["","","Grijanje","","B"]
["Učin grijanja","Nom.","","kW","10.8"]
["Napomene","","","","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU"]
["","","","","(2) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja"]