{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / AZAS-MV1"]
[]
[]
[]
[]
["","","","","FBA71A2VEB / AZAS71M2V1B (Archived)"]
["Outdoor unit","","","","AZAS71M2V1B"]
["Učin hlađenja","Nom.","","kW","6.80"]
["Učin grijanja","Nom.","","kW","7.50"]
["Hlađenje prostora","Razred energetske učinkovitosti","","","A"]
["","Kapacitet","Pdesign","kW","6.80"]
["","SEER","","","5.57"]
["","Godišnja potrošnja energije","","kWh/a","427"]
["Grijanje prostora (prosječna klima)","Razred energetske učinkovitosti","","","A"]
["","Kapacitet","Pdesign","kW","4.50"]
["","SCOP/A","","","3.81"]
["","Godišnja potrošnja energije","","kWh/a","1654"]
["Napomene","","","","(1) - Hlađenje: T2: unutarnja temperatura 26,6 °C DB, 19,4 °C WB, vanjska temperatura: 48 °CDB [Btu/hr/W]"]
["","","","","(2) - Nazivni učin grijanja zasnovani su na: unutarnja temperatura: 20°C DB, vanjska temperatura : 7°C DB, 6°C WB, odgovarajući cjevovod za radnu tvar: 5 m, razlika razine: 0 m."]