{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / ARXM-N9"]
[]
[]
[]
[]
["","","","","FCAG71BVEB / ARXM71N2V1B9"]
["Učin hlađenja","Nom.","","kW","6.80"]
["","Maks.","","kW","7.05"]
["Učin grijanja","Nom.","","kW","7.50"]
["","Maks.","","kW","7.58"]
["Nazivna učinkovitost","Godišnja potrošnja energije","","kWh","1,083"]
["","COP","","","3.38"]
["","EER","","","3.14"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","B"]
["","","Grijanje","","C"]
["Napomene","","","","(1) - Pogledajte odvojene nacrte za radno područje"]
["","","","","(2) - Vidi električne podatke na posebnim nacrtima"]
["","","","","(3) - Nom. kapacitet hlađenja se temelji se na sljedećim parametrima: unutarnja temperatura: 27 °C DB, 19 °C WB, vanjska temperatura: 35 °C DB, odgovarajuće cijevi rashladnog sredstva: 5 m, razlika u visini: 0m."]
["","","","","(4) - Nazivni učin grijanja zasnovani su na: unutarnja temperatura: 20°C DB, vanjska temperatura : 7°C DB, 6°C WB, odgovarajući cjevovod za radnu tvar: 5 m, razlika razine: 0 m."]