{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":13,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-H / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100HVEB / RZQG100L8Y1B","FCAHG125HVEB / RZQG125L8Y1B","FCAHG140HVEB / RZQG100L8Y1B","FCAHG140HVEB / RZQG125L8Y1B","FCAHG71HVEB / FCAHG71HVEB / RZQG100L8Y1B","FCAHG71HVEB / FCAHG71HVEB / RZQG125L8Y1B","FCAHG100HVEB / RZQG71L8Y1B","FCAHG71HVEB / RZQG71L8Y1B","FCAHG140HVEB / RZQG140L7Y1B"]
["Raspon energetske učinkovitosti","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Učin hlađenja","Nom.","","kW","","","","","","","6.80","6.80","13.40"]
["Hlađenje prostora","SEER","","","","","","","","","6.91","6.91","6.75"]
["","Godišnja potrošnja energije","","kWh/a","","","","","","","345","345","1,191"]
["","Kapacitet","Pdesign","kW","","","","","","","6.80","6.80","13.40"]
["","Razred energetske učinkovitosti","","","","","","","","","A++","A++"]
["Grijanje prostora (prosječna klima)","Kapacitet","Pdesign","kW","","","","","","","7.60","7.60","11.78"]
["","SCOP/A","","","","","","","","","4.54","4.54","4.38"]
["","Razred energetske učinkovitosti","","","","","","","","","A+","A+"]
["","Godišnja potrošnja energije","","kWh/a","","","","","","","2,344","2,344","3,766"]
["Nazivna učinkovitost","EER","","","","","","","","","4.09","4.09","3.18"]
["Napomene","","","","","","","","","","(1) - Pogledajte odvojene nacrte za radno područje","(1) - Nominalan kapacitet hlađenja se temelji se na sljedećim parametrima: unutarnja temperatura: 27 °C DB, 19 °C WB, vanjska temperatura: 35 °C DB, odgovarajuće cijevi rashladnog sredstva: 5 m, razlika u visini: 0m.","(1) - Nominalan kapacitet hlađenja se temelji se na sljedećim parametrima: unutarnja temperatura: 27 °C DB, 19 °C WB, vanjska temperatura: 35 °C DB, odgovarajuće cijevi rashladnog sredstva: 5 m, razlika u visini: 0m."]
["","","","","","","","","","","(2) - Vidi električne podatke na posebnim nacrtima","(2) - Nazivni učin grijanja zasnovani su na: unutarnja temperatura: 20°C DB, vanjska temperatura : 7°C DB, 6°C WB, odgovarajući cjevovod za radnu tvar: 5 m, razlika razine: 0 m.","(2) - Nazivni učin grijanja zasnovani su na: unutarnja temperatura: 20°C DB, vanjska temperatura : 7°C DB, 6°C WB, odgovarajući cjevovod za radnu tvar: 5 m, razlika razine: 0 m."]
["Nazivna učinkovitost","Godišnja potrošnja energije","","kWh","","","","","","","","831"]
["","COP","","","","","","","","","","4.80","4.12"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","","","","","","","","A"]
["","","Grijanje","","","","","","","","","A"]
["Učin grijanja","Nom.","","kW","","","","","","","","7.50","15.50"]
["Napomene","","","","","","","","","","","(3) - Pogledajte odvojene nacrte za radno područje","(3) - Pogledajte odvojene nacrte za radno područje"]
["","","","","","","","","","","","(4) - Vidi električne podatke na posebnim nacrtima","(4) - Vidi električne podatke na posebnim nacrtima"]
["Hlađenje prostora","ηs,c","","%","","","","","","","","","266.88"]
["Grijanje prostora (prosječna klima)","ηs,h","","%","","","","","","","","","172.10"]