{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":12,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCQG100FVEB / RZQSG100L8Y1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG100L8Y1B","FCQG50FVEB / FCQG50FVEB / RZQSG100L8Y1B","FCQG125FVEB / RZQSG125L8Y1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG125L8Y1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQSG125L8Y1B","FCQG60FVEB / FCQG60FVEB / RZQSG125L8Y1B","FCQG140FVEB / RZQSG140L7Y1B"]
["Učin hlađenja","Nom.","","kW","9.5","","","12.0","","","","13.4"]
["Hlađenje prostora","SEER","","","6.5","5.1","5.1","5.3","4.8","4.8","4.8"]
["","Godišnja potrošnja energije","","kWh/a","512","652","652","793","875","875","875"]
["","Kapacitet","Pdesign","kW","9.5","9.5","9.5","12","12","12","12"]
["","Razred energetske učinkovitosti","","","A++","B","B","A","B","B","B"]
["Grijanje prostora (prosječna klima)","Kapacitet","Pdesign","kW","7.6","7.6","7.6","8.03","7.6","7.6","7.6"]
["","SCOP/A","","","4.1","3.8","3.8","4.01","3.8","3.8","3.8"]
["","Razred energetske učinkovitosti","","","A+","A","A","A+","A","A","A"]
["","Godišnja potrošnja energije","","kWh/a","2,596","2,800","2,800","2,804","2,800","2,800","2,800"]
["Nazivna učinkovitost","Godišnja potrošnja energije","","kWh","1,440","","","1,870","","","","2,225"]
["","EER","","","3.30","","","3.21","","","","3.01"]
["","COP","","","3.54","","","3.41","","","","3.41"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","A","","","A"]
["","","Grijanje","","A","","","B"]
["Učin grijanja","Nom.","","kW","10.8","","","13.5","","","","15.5"]
["Napomene","","","","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","","","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","","","","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU"]
["","","","","(2) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja","","","(2) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja","","","","(2) - Nazivna učinkovitost: hlađenje na 35°/27° nazivnog opterećenja, grijanje na 7°/20° nazivnog opterećenja"]
["","","","","(3) - Godišnja potrošnja energije u skladu je s direktivom oznake energetske učinkovitosti 2002/31/EC","","","(3) - Godišnja potrošnja energije u skladu je s direktivom oznake energetske učinkovitosti 2002/31/EC"]
["","","","","(4) - SEER i SCOP su u skladu s EN 14825","","","(4) - SEER i SCOP su u skladu s EN 14825"]
["","","","","","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU","(1) - EER/COP prema Eurovent 2012, za korištenje samo izvan EU"]