{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Učin hlađenja","Ukupan učin","","Nom.","kW","12.10","19.00","22.00"]
["Kapacitet grijanja","Ukupni učin","","Nom.","kW","13.50","22.4","24.0"]
["Kućište","Boja","","","","Neobojano","Neobojano","Neobojano"]
["","Materijal","","","","Galvanizirani čelik","Galvanizirana čelična ploča","Galvanizirana čelična ploča"]
["Dimenzije","Uređaj","","Visina","mm","300","470","470"]
["","","","Širina","mm","1,400","1,490","1,490"]
["","","","Dubina","mm","700","1,100","1,100"]
["Težina","Uređaj","","","kg","45","104","115"]
["Potreban otvor u stropu >","mm","","","","350"]
["Ventilator","Količina zraka","Hlađenje","Visoko","m³/min","39.0","64.0","69.0"]
["","","","Srednji","m³/min","","50","56"]
["","","","Nizak","m³/min","28.0","36.0","43.0"]
["","","Grijanje","Visoko","m³/min","39.0","64.0","69.0"]
["","","","Srednji","m³/min","","50.0","56.0"]
["","","","Nizak","m³/min","28.0","36.0","43.0"]
["","Vanjski statički tlak","","Visoki","Pa","200","250","250"]
["","","","Nom.","Pa","50","62","62"]
["Sound power level","Hlađenje","","","dBA","66","69.0","71.0"]
["Razina tlaka zvuka","Hlađenje","","Visoko","dBA","40","43.0","44.0"]
["","","","Srednji","dBA","","39.0","40.0"]
["","","","Nizak","dBA","33","36.0","37.0"]
["","Grijanje","","Visoko","dBA","40","43.0","44.0"]
["","","","Srednji","dBA","","39.0","40.0"]
["","","","Nizak","dBA","33","36.0","37.0"]
["Priključci cjevovoda","Tekućina","","VP","mm","9.52","9.52","9.52"]
["","Plin","","VP","mm","15.90","19.1","22.2"]
["","Odvod vode","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Odvod do visine","mm","","","","625"]
["Dekorativni panel","Model","","","","BYBS125DJW1"]
["","Boja","","","","Bijelo (10Y9/0.5)"]
["","Dimenzije","","Visina","mm","55"]
["","","","Širina","mm","1,500"]
["","","","Dubina","mm","500"]
["","Težina","","","kg","6.5"]
["Control systems","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standardna dodatna oprema","Vijci","","","","16","2","2"]
["","Podloška","","","","8","12","12"]
["","Traka za crijevo","","","","1"]
["","Drenažno crijevo","","","","1"]
["","Opće mjere sigurnosti","","","","1","1","1"]
["","Priručnik za instalaciju i rukovanje","","","","1","1","1"]
["","Vod za zajedničko električno napajanje","","","","2"]
["","Brtveni materijal (crijevo za odvod kondenzata)","","","","1"]
["","Materijal za brtvljenje","","","","2"]
["","Cijev s toplinskom izolacijom (tekućina)","","","","1"]
["","Cijev s toplinskom izolacijom (plin)","","","","1"]
["Power supply","Naziv","","","","","VE","VE"]
["","Faza","","","","1~","1~","1~"]
["","Frekvencija","","","Hz","50/60","50/60","50/60"]
["","Napon","","","V","220-240/220","220-240/220","220-240/220"]
["Napomene","","","","","(1) - Vidi električne podatke na posebnim nacrtima"]
["Standardna dodatna oprema","Radni priručnik","","","","","1","1"]
["","Priručnik za instalaciju","","","","","1","1"]
["","Spojna plinska cijev","","","","","1","1"]
["","Materijal stezaljke žice","","","","","1","1"]
["","Opružna podloška","","","","","2","2"]
["","Vijak+podloška","","","","","45","45"]
["","Vijak s šesterokutnom glavom s podloškom","","","","","49","49"]
["","Vijak s šesterokutnom glavom","","","","","2","2"]
["","Ravna podloška","","","","","8","8"]