{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDBQ-B"]
[]
[]
[]
[]
["","","","","","FDBQ25B5V1","FDBQ25B8V1"]
["Razina tlaka zvuka","Grijanje","","Visoko","dBA","35.0","35.0"]
["","","","Nizak","dBA","29.0","29.0"]
["","Hlađenje","","Nizak","dBA","28.0","28.0"]
["","","","Visoko","dBA","35.0","35.0"]
["Standardna dodatna oprema","Priručnik za instalaciju i rukovanje","","","","1","1"]
["","Filtar usisnog zraka","","","","1","1"]
["Upravljački sustavi","Žično daljinsko upravljanje","","","","BRC1D52, BRC1E52A/B"]
["Priključci cjevovoda","Tekućina","","VP","mm","6.35"]
["","Plin","","VP","mm","9.52"]
["","Odvod vode","","","","27.2"]
["Zvučna snaga","Hlađenje","","","dBA","55","55"]
["","Grijanje","","","dBA","55","55"]
["Dimenzije","Uređaj","","Širina","mm","652","652"]
["","","","Dubina","mm","502","502"]
["","","","Height","mm","230","230"]
["Kućište","Materijal","","","","Pocinčani niskougljični čelik","Pocinčani niskougljični čelik"]
["Težina","Uređaj","","","kg","17.0","17.0"]
["Ventilator","Brzina protoka zraka","Grijanje","Visoko","m³/min","","6.95"]
["","","","Nizak","m³/min","","5.20"]
["","","Hlađenje","Nizak","m³/min","","5.20"]
["","","","Visoko","m³/min","","6.50"]
["Power supply","Phase","","","","1~","1~"]
["","Frekvencija","","","Hz","50","50"]
["","Naziv","","","","V1","V1"]
["","Napon","","","V","230","230 +/-10%"]
["Napomene","","","","","(1) - Vrijednosti zvuka mjere se u prostoriji s poluodjekom.","(1) - Vrijednosti zvuka mjere se u prostoriji s poluodjekom."]
["","","","","","(2) - Razina tlaka zvuka je relativna vrijednost, ovisno o udaljenosti i akustici okoliša. Za više detalja molimo vas da pogledate nacrte o razini zvuka.","(2) - Razina tlaka zvuka je relativna vrijednost, ovisno o udaljenosti i akustici okoliša. Za više detalja molimo vas da pogledate nacrte o razini zvuka."]
["","","","","","(3) - Razina jačine zvuka apsolutna je vrijednost koja označava snagu koju generira izvor zvuka.","(3) - Razina jačine zvuka apsolutna je vrijednost koja označava snagu koju generira izvor zvuka."]
["Priključci cjevovoda","Tekućina","","VP","mm","","6.35"]
["","Plin","","VP","mm","","9.52"]
["","Odvod vode","","","","","27.2"]