{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":6,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / 2MXM-M"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B / FDXM25F3V1B / 2MXM40M3V1B","FDXM25F3V1B / FDXM35F3V1B / 2MXM40M3V1B"]
["Učin hlađenja","Nom.","","kW","4.0","4.0"]
["Nazivna učinkovitost","Godišnja potrošnja energije","","kWh","563","555"]
["","EER","","","3.55","3.60"]
["","COP","","","4.13","4.17"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","A","A"]
["","","Grijanje","","A","A"]
["Učin grijanja","Nom.","","kW","4.20","4.20"]
["Napomene","","","","(1) - Nazivni učini hlađenja se temelje na: unutarnjoj temperaturi: 27 °CDB, 19 °CWB, vanjskoj temperaturi: 35 °CDB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju standardne učinkovitosti","(1) - Nazivni učini hlađenja se temelje na: unutarnjoj temperaturi: 27 °CDB, 19 °CWB, vanjskoj temperaturi: 35 °CDB, ekvivalentnom cjevovodu radne tvari: 5 m, razlici u visini: 0 m. Podaci za seriju standardne učinkovitosti"]
["","","","","(2) - Nazivni učin grijanja zasnovani su na: unutarnja temperatura: 20°C DB, vanjska temperatura : 7°C DB, 6°C WB, odgovarajući cjevovod za radnu tvar: 5 m, razlika razine: 0 m.","(2) - Nazivni učin grijanja zasnovani su na: unutarnja temperatura: 20°C DB, vanjska temperatura : 7°C DB, 6°C WB, odgovarajući cjevovod za radnu tvar: 5 m, razlika razine: 0 m."]