{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":8,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RXM-M9"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B / RXM25M3V1B9","FDXM35F3V1B / RXM35M3V1B9","FDXM50F3V1B / RXM50M3V1B9","FDXM60F3V1B / RXM60M3V1B9"]
["Učin hlađenja","Min.","","kW","","1.40","","1.70"]
["","Maks.","","kW","","3.80","","6.50"]
["","Nom.","","kW","","3.40","","6.00"]
["Hlađenje prostora","SEER","","","","5.26","","5.56"]
["","Godišnja potrošnja energije","","kWh/a","","226","","315"]
["","Kapacitet","Pdesign","kW","","3.40","","6.00"]
["","Razred energetske učinkovitosti","","","","A","","A"]
["Grijanje prostora (prosječna klima)","Kapacitet","Pdesign","kW","","2.90","","4.60"]
["","SCOP/A","","","","3.88","","3.80"]
["","Razred energetske učinkovitosti","","","","A","","A"]
["","Godišnja potrošnja energije","","kWh/a","","1,046","","1,693"]
["Nazivna učinkovitost","Godišnja potrošnja energije","","kWh","","570","","1,024"]
["","EER","","","","2.98","","2.93"]
["","COP","","","","3.48","","3.21"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","","C","","C"]
["","","Grijanje","","","B","","C"]
["Učin grijanja","Nom.","","kW","","4.00","","7.00"]
["","Min.","","kW","","1.40","","1.70"]
["","Maks.","","kW","","5.00","","7.10"]
["Napomene","","","","","(1) - Vidi električne podatke na posebnim nacrtima","","(1) - Pogledajte odvojene nacrte za radno područje"]
["","","","","","(2) - Pogledajte odvojene nacrte za radno područje","","(2) - Vidi električne podatke na posebnim nacrtima"]
["","","","","","(3) - Nom. kapacitet hlađenja se temelji se na sljedećim parametrima: unutarnja temperatura: 27 °C DB, 19 °C WB, vanjska temperatura: 35 °C DB, odgovarajuće cijevi rashladnog sredstva: 5 m, razlika u visini: 0m.","","(3) - Nom. kapacitet hlađenja se temelji se na sljedećim parametrima: unutarnja temperatura: 27 °C DB, 19 °C WB, vanjska temperatura: 35 °C DB, odgovarajuće cijevi rashladnog sredstva: 5 m, razlika u visini: 0m."]
["","","","","","(4) - Nazivni učin grijanja zasnovani su na: unutarnja temperatura: 20°C DB, vanjska temperatura : 7°C DB, 6°C WB, odgovarajući cjevovod za radnu tvar: 5 m, razlika razine: 0 m.","","(4) - Nazivni učin grijanja zasnovani su na: unutarnja temperatura: 20°C DB, vanjska temperatura : 7°C DB, 6°C WB, odgovarajući cjevovod za radnu tvar: 5 m, razlika razine: 0 m."]
["Outdoor unit","","","","RXM25M3V1B9","","RXM50M3V1B9"]
["Učin hlađenja","Min.","","kW","1.30","","1.70"]
["","Nom.","","kW","2.40","","5.00"]
["","Maks.","","kW","3.00","","5.30"]
["Učin grijanja","Min.","","kW","1.30","","1.70"]
["","Nom.","","kW","3.20","","5.80"]
["","Maks.","","kW","4.50","","6.00"]
["Nazivna učinkovitost","EER","","","3.77","","3.06"]
["","COP","","","4.00","","3.10"]
["","Godišnja potrošnja energije","","kWh","318","","816"]
["","Direktiva o označivanju energetske učinkovitosti","Hlađenje","","A","","B"]
["","","Grijanje","","A","","D"]
["Hlađenje prostora","Razred energetske učinkovitosti","","","A+","","A+"]
["","Kapacitet","Pdesign","kW","2.40","","5.00"]
["","SEER","","","5.68","","5.77"]
["","Godišnja potrošnja energije","","kWh/a","148","","303"]
["Grijanje prostora (prosječna klima)","Razred energetske učinkovitosti","","","A+","","A"]
["","Kapacitet","Pdesign","kW","2.60","","4.00"]
["","SCOP/A","","","4.24","","3.93"]
["","Pdh kapacitet grijanja pri -10°","","kW","2.16","","3.55"]
["","Godišnja potrošnja energije","","kWh/a","858","","1424"]