{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B","FDXM35F3V1B","FDXM50F3V1B","FDXM60F3V1B"]
["Razina tlaka zvuka","Grijanje","Visoko","dBA","35","35","38","38"]
["","","Srednji","dBA","33","33","35","35"]
["","","Nizak","dBA","27","27","30","30"]
["","Hlađenje","Srednji","dBA","33","33","35","35"]
["","","Nizak","dBA","27","27","30","30"]
["","","Visoko","dBA","35","35","38","38"]
["Standardna dodatna oprema","Priručnik za instalaciju","","","1","1","1","1"]
["","Radni priručnik","","","1","1","1","1"]
["","Izolacija priključka","","","1","1","1","1"]
["","Umetak za brtvljenje","","","1","1","1","1"]
["","Metalna stezaljka","","","1","1","1","1"]
["","Drenažno crijevo","","","1","1","1","1"]
["","Podloška za okvir vješalice","","","8","8","8","8"]
["","Materijal za brtvljenje","","","2","2","2","2"]
["","Stezaljke","","","6","6","6","6"]
["","Ploča za fiksiranje podloški","","","4","4","4","4"]
["","Vijci za prirubnice vodova","","","1","1","1","1"]
["","Zračni filtar","","","1","1","1","1"]
["Priključci cjevovoda","Tekućina","VP","mm","6.35","6.35","6.35","6.35"]
["","Plin","VP","mm","9.50","9.50","12.70","12.70"]
["","Odvod vode","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Ulazna struja","Hlađenje","Nom.","kW","0.036","0.036","0.060","0.060"]
["","Grijanje","Nom.","kW","0.036","0.036","0.060","0.060"]
["Sound power level","Hlađenje","","dBA","53","53","55","56"]
["","Grijanje","","dBA","53","53","55","56"]
["Dimenzije","Uređaj","Širina","mm","750","750","1,150","1,150"]
["","","Dubina","mm","620","620","620","620"]
["","","Visina","mm","200","200","200","200"]
["Težina","Uređaj","","kg","21","21","28","28"]
["Ventilator","Vanjski statički tlak","Nom.","Pa","30","30","40","40"]
["Power supply","Faza","","","1~","1~","1~","1~"]
["","Frekvencija","","Hz","50","50","50","50"]
["","Napon","","V","220-240","220-240","220-240","220-240"]